;; netrtwlanu.inf 
;;
;; Realtek Wireless 802.11b/g/n USB 2.0 Network Adapter
;;
;; Copyright (C) 2012 Realtek Semiconductor Corp.
;;
;; This release is primarily for WHQL test.
;;

;; FOR XP/Vista/Win7/Win8

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%
CatalogFile.NT	= netrtwlanu.cat		;; for WHQL certified
DriverVer = 12/25/2017,1030.25.0701.2017

[Manufacturer]
%Realtek% = Realtek,NTx86.6.3

[ControlFlags]
ExcludeFromSelect = *

[Realtek.NTx86.6.3]

;; For 8188E RTK common		================================================================
%RTL8188eu.DeviceDesc%  			= RTL8188eu.ndi, 	USB\VID_0BDA&PID_8179
%RTL8188eu.DeviceDesc%  			= RTL8188eu.ndi, 	USB\VID_0BDA&PID_8179&REV_0200&SS
%RTL8188ee_vau.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_A179
%RTL8188ee_vau.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_A179&REV_0200&SS
%RTL8188eu_0179.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_0179
%RTL8188eu_0179.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_0179&REV_0200&SS

;; For 8812A RTK common		================================================================
%RTL8812au.DeviceDesc% 				= RTL8812au.ndi, 	USB\VID_0BDA&PID_8812
%RTL8812au.DeviceDesc% 				= RTL8812au.ndi, 	USB\VID_0BDA&PID_A812
%RTL8812au_881A.DeviceDesc% 		= Vx_RTL8812au.ndi, USB\VID_0BDA&PID_881A
%RTL8812au_881B.DeviceDesc% 		= Vx_RTL8812au.ndi, USB\VID_0BDA&PID_881B
%RTL8812au_881C.DeviceDesc% 		= Vx_RTL8812au.ndi, USB\VID_0BDA&PID_881C

;; For 8811A RTK common		================================================================
%RTL8811au.DeviceDesc% 					= RTL8811au.ndi, 			USB\VID_0BDA&PID_0811
%RTL8811au.DeviceDesc% 					= RTL8811au.ndi, 			USB\VID_0BDA&PID_A811
%RTL8811au.DeviceDesc% 					= RTL8811au.ndi, 			USB\VID_7392&PID_A813
%RTL8811au_Combo.DeviceDesc% 			= LC_RTL8821au.ndi, 		USB\VID_0BDA&PID_0823&MI_02
%RTL8811au_Combo.DeviceDesc% 			= LC_RTL8821au.ndi, 		USB\VID_0BDA&PID_0823&REV_0200&MI_02
%RTL8811au_Combo.DeviceDesc% 			= LC_RTL8821au.ndi, 		USB\VID_0BDA&PID_0170&MI_02
%IO_DATA_2003.DeviceDesc% 				= 5GOnly_RTL8811au.ndi, 	USB\VID_0BDA&PID_2003

;; For 8192E RTK common		================================================================
%RTL8192eu.DeviceDesc% 				= RTL8192eu.ndi, 	USB\VID_0BDA&PID_818B
%RTL8192eu.DeviceDesc% 				= RTL8192eu.ndi, 	USB\VID_0BDA&PID_818C&MI_02
%RTL8192eu.DeviceDesc% 				= RTL8192eu.ndi, 	USB\VID_0BDA&PID_818C&REV_0200&MI_02			

;;----------------------------------------------------------------------------
;; For 8822B RTK common
;;----------------------------------------------------------------------------
%RTL8822bu.DeviceDesc%		= RTL8822bu.ndi,		USB\VID_0BDA&PID_B82C&MI_02
%RTL8822bu.DeviceDesc%		= RTL8822bu.ndi,		USB\VID_0BDA&PID_B82C&REV_0200&MI_02
%RTL8822bu.DeviceDesc%		= RTL8822bu.ndi,		USB\VID_0BDA&PID_B82C&REV_0201&MI_02
%RTL8822bu.DeviceDesc%		= RTL8822bu.ndi,		USB\VID_0BDA&PID_B82C&REV_0210&MI_02
%RTL8822bu.DeviceDesc%		= RTL8822bu.ndi,		USB\VID_0BDA&PID_B82C&REV_0300&MI_02
%RTL8812bu.DeviceDesc%		= RTL8812bu.ndi,		USB\VID_0BDA&PID_B812
%RTL8812bu.DeviceDesc%		= RTL8812bu.ndi,		USB\VID_0BDA&PID_B81A


;;----------------------------------------------------------------------------
;; For 8821C RTK common
;;----------------------------------------------------------------------------
%RTL8821cu.DeviceDesc%		= RTL8821cu.ndi,		USB\VID_0BDA&PID_C820&MI_02

;;----------------------------------------------------------------------------
;; For 8811C RTK common
;;----------------------------------------------------------------------------
%RTL8811cu.DeviceDesc%		= RTL8811cu.ndi,		USB\VID_0BDA&PID_C82B
%RTL8811cu.DeviceDesc%		= RTL8811cu.ndi,		USB\VID_0BDA&PID_C811
%ZION_2006.DeviceDesc%		= RTL8811cu.ndi,		USB\VID_0BDA&PID_2006

;;----------------------------------------------------------------------------
;; For 8814A RTK common
;;----------------------------------------------------------------------------
%RTL8814au.DeviceDesc% 				= RTL8814au.ndi, 	USB\VID_0BDA&PID_8813

;;----------------------------------------------------------------------------
;; For 8723B RTK common
;;----------------------------------------------------------------------------
%RTL8723bu.DeviceDesc% 				= RTL8723bu.ndi, 	USB\VID_0BDA&PID_B720&MI_02
%RTL8723bu.DeviceDesc% 				= RTL8723bu.ndi, 	USB\VID_0BDA&PID_B720&REV_0200&MI_02

;; For 8703 RTK common		================================================================
%RTL8703bu.DeviceDesc%  			= RTL8703bu.ndi, 	USB\VID_0BDA&PID_B703&MI_02

;;----------------------------------------------------------------------------
;; For 8188F RTK common
;;----------------------------------------------------------------------------
%RTL8188fu.DeviceDesc% 				= RTL8188fu.ndi, 	USB\VID_0BDA&PID_F179


;; For 8723D RTK common		================================================================
%RTL8723du.DeviceDesc% 				= RTL8723du.ndi, 	USB\VID_0BDA&PID_D72B
%RTL8723du.DeviceDesc% 				= RTL8723du.ndi,	USB\VID_0BDA&PID_D723&REV_0200&MI_02
%RTL8723du.DeviceDesc% 				= RTL8723du.ndi, 	USB\VID_0BDA&PID_D723&MI_02

;; For 8710B RTK common		================================================================
%RTL8710bu.DeviceDesc% 				= RTL8710bu.ndi, 	USB\VID_0BDA&PID_B711
%ZION_2005.DeviceDesc% 				= RTL8710bu.ndi, 	USB\VID_0BDA&PID_2005

;; For 8812A ASUS			================================================================
%ASUS_17D2.DeviceDesc% 			= ASUS_RTL8812au.ndi, 		USB\VID_0B05&PID_17D2

;; For 8814A ASUS			================================================================
%ASUS_1817.DeviceDesc% 			= ASUS_RTL8814au.ndi, 	USB\VID_0B05&PID_1817
%ASUS_1852.DeviceDesc% 			= ASUS_RTL8814au.ndi, 	USB\VID_0B05&PID_1852
%ASUS_1853.DeviceDesc% 			= ASUS_RTL8814au.ndi, 	USB\VID_0B05&PID_1853

;; For 8822B ASUS
%ASUS_1841.DeviceDesc%		= EXT_RTL8812bu.ndi,		USB\VID_0B05&PID_1841
%ASUS_184C.DeviceDesc%		= U2_RTL8812bu.ndi,		USB\VID_0B05&PID_184C
%ASUS_1870.DeviceDesc%		= RTL8812bu.ndi,		USB\VID_0B05&PID_1870
%ASUS_1874.DeviceDesc%		= RTL8812bu.ndi,		USB\VID_0B05&PID_1874

;;----------------------------------------------------------------------------
;; Realtek 8723bu default installation
;;----------------------------------------------------------------------------

             


[RTL8723bu.ndi.NT]
AddReg				= NDIS_63.reg, RTL8723b_common.reg, 11nWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, ConnectedStandbyEnable.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, BandWidthSetting.reg, NdisSS.reg, PnpPreTransOn.reg, LPSOn.reg, IPSOn.reg, DisableSS.reg


Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8723bu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8723bu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;----------------------------------------------------------------------------
;; Realtek 8703bu default installation
;;----------------------------------------------------------------------------

             


[RTL8703bu.ndi.NT]
AddReg				= NDIS_63.reg, RTL8723_common.reg, 11nWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, ConnectedStandbyEnable.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, BandWidthSetting.reg, NdisSS.reg, PnpPreTransOn.reg, LPSOn.reg, IPSOn.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8703bu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8703bu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;----------------------------------------------------------------------------
;; Realtek 8188eu default installation
;;----------------------------------------------------------------------------




[RTL8188eu.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg.reg, RtlSsOnn.reg, 11nWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg


Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8188eu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8188eu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




;;----------------------------------------------------------------------------
;; Realtek 8188eu disable TX power training installation
;;----------------------------------------------------------------------------




[TplinkDisTxPwrTrain_RTL8188eu.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg.reg, RtlSsOnn.reg, 11nWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, DisableTxPowerTraining.reg


Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[TplinkDisTxPwrTrain_RTL8188eu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[TplinkDisTxPwrTrain_RTL8188eu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;----------------------------------------------------------------------------
;; Realtek 8188fu default installation
;;----------------------------------------------------------------------------

             


[RTL8188fu.ndi.NT]
AddReg				= NDIS_63.reg, RTL8188fu.common.reg, Ndis6UsbRxAgg_Jaguar.reg, 11nWirelessMode.reg, ConnectedStandbyEnable.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, BandWidthSetting.reg, NdisSS.reg, PnpPreTransOn.reg, LPSOn.reg, IPSOn.reg, MCCDisable.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8188fu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8188fu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;----------------------------------------------------------------------------
;; Realtek 8811AU default installation
;;----------------------------------------------------------------------------




[RTL8811au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, 11acWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOff.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg , RTL8811AU_COMMON.reg, TcpReorderEnable.reg, ScanType.reg


Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8811au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8811au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration







[Disable8021X_RTL8811au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, 11acWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOff.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg , RTL8811AU_COMMON.reg, TcpReorderEnable.reg, ScanType.reg, Disable8021X_WifiConfig.reg


Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[Disable8021X_RTL8811au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[Disable8021X_RTL8811au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration







[LC_RTL8821au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, 11acWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOff.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8821AU.reg, RTL8811AU_COMMON.reg, TcpReorderEnable.reg, ScanType.reg, WowlanEnableNoLPSNoPatternMatch.reg, DisableSS.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[LC_RTL8821au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[LC_RTL8821au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration







[PCI_RTL8811au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, 5G11acWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOff.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg , RTL8811AU_COMMON.reg, TcpReorderEnable.reg, ScanType.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[PCI_RTL8811au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[PCI_RTL8811au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration







[5GOnly_RTL8811au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, 5G11acWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOff.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg , RTL8811AU_COMMON.reg, TcpReorderEnable.reg, ScanType.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[5GOnly_RTL8811au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[5GOnly_RTL8811au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




;;----------------------------------------------------------------------------
;; Realtek 8812AU default installation
;;----------------------------------------------------------------------------




[RTL8812au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTL8812au.common.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, USBSwitch.reg, ScanType.reg, VHT24G.reg,HAdhoc.reg,KFREE_COMMON.reg


Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration







[Vx_RTL8812au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, USBModeVx.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, ScanType.reg,VHT24G.reg,HAdhoc.reg,KFREE_COMMON.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71         ; IF_TYPE_IEEE80211
*MediaType			= 16         ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[Vx_RTL8812au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[Vx_RTL8812au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration







[Belkin_RTL8812au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTL8812au.common.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomerID_Belkin.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, USBSwitch.reg, ScanType.reg,VHT24G.reg,HAdhoc.reg,KFREE_COMMON.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[Belkin_RTL8812au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[Belkin_RTL8812au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration







[tplink_RTL8812au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTL8812au.common.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, USBSwitch3.reg,KFREE_COMMON.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[tplink_RTL8812au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[tplink_RTL8812au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration







[DLink_RTL8812au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTL8812au.common.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomerID_DLink.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, USBSwitch.reg, ScanType.reg,VHT24G.reg,HAdhoc.reg,KFREE_COMMON.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[DLink_RTL8812au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[DLink_RTL8812au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;----------------------------------------------------------------------------
;; NEC 8812AU default installation
;;----------------------------------------------------------------------------




[NEC_RTL8812au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, CustomerID_NEC.reg, NEC.reg, Signal.reg, sifs.reg, USBSwitch.reg, ScanType.reg,KFREE_COMMON.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[NEC_RTL8812au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[NEC_RTL8812au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration







[ASUS_RTL8812au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTL8812au.common.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomerID_ASUS.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, USBSwitch.reg, ScanType.reg,VHT24G.reg,HAdhoc.reg,KFREE_COMMON.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[ASUS_RTL8812au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[ASUS_RTL8812au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




;;----------------------------------------------------------------------------
;;----------------------------------------------------------------------------




[RTL8192eu.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, 11nWirelessMode.reg, RtlSsOff.reg,TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg , RTL8192EU_COMMON.reg, TcpReorderEnable.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192eu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8192eu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration







[DLINK_RTL8192eu.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, 11nWirelessMode.reg, RtlSsOff.reg,TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg , DLINK_RTL8192EU_COMMON.reg, TcpReorderEnable.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[DLINK_RTL8192eu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[DLINK_RTL8192eu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




;;----------------------------------------------------------------------------
;; Realtek 8814AU default installation
;;----------------------------------------------------------------------------




[RTL8814au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, RTL8814au.common.reg,KFREE_COMMON.reg,VHT24G.reg


Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8814au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8814au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




;;----------------------------------------------------------------------------
;; EdiMax 8814AU 3T3R installation
;;----------------------------------------------------------------------------




[3T3R_RTL8814au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, RTL8814au3T3R.common.reg,KFREE_COMMON.reg,VHT24G.reg


Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[3T3R_RTL8814au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[3T3R_RTL8814au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




;;----------------------------------------------------------------------------
;; ELECOM 8814AU 3T3R 5G only installation
;;----------------------------------------------------------------------------




[3T3R_5GOnly_RTL8814au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 5G11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, RTL8814au3T3R.common.reg,KFREE_COMMON.reg,VHT24G.reg


Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[3T3R_5GOnly_RTL8814au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[3T3R_5GOnly_RTL8814au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




;;----------------------------------------------------------------------------
;; Dlink 8814AU installation
;;----------------------------------------------------------------------------




[DLink_RTL8814au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, RTL8814au.common.reg, CustomerID_DLink.reg,KFREE_COMMON.reg,VHT24G.reg


Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[DLink_RTL8814au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[DLink_RTL8814au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




;;----------------------------------------------------------------------------
;; ASUS 8814AU installation
;;----------------------------------------------------------------------------




[ASUS_RTL8814au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, RTL8814au.common.reg, CustomerID_ASUS.reg,KFREE_COMMON.reg,VHT24G.reg


Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[ASUS_RTL8814au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[ASUS_RTL8814au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




;;----------------------------------------------------------------------------
;; TREND_NET 8814AU installation
;;----------------------------------------------------------------------------




[TREND_RTL8814au.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, RTL8814au.common.reg,KFREE_COMMON.reg,VHT24G.reg,CustomerLED8814A_TREND.reg


Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[TREND_RTL8814au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[TREND_RTL8814au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




;;----------------------------------------------------------------------------
;; Realtek 8822BU default installation
;;----------------------------------------------------------------------------




[RTL8822bu.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, RTL8822bu.common.reg, VHT24G.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8822bu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8822bu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;----------------------------------------------------------------------------
;; Realtek 8812BU (iPA forced U2)default installation
;;----------------------------------------------------------------------------




[U2_RTL8812bu.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, U2_RTL8812bu.common.reg, VHT24G.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[U2_RTL8812bu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[U2_RTL8812bu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




;;----------------------------------------------------------------------------
;; Realtek 8812BU (Internal PA)default installation
;;----------------------------------------------------------------------------




[RTL8812bu.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, RTL8812bu.common.reg, VHT24G.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812bu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812bu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;----------------------------------------------------------------------------
;; Realtek 8812BU (Internal PA)default installation
;;----------------------------------------------------------------------------




[Belkin_RTL8812bu.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, Belkin_RTL8812bu.common.reg, VHT24G.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[Belkin_RTL8812bu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[Belkin_RTL8812bu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;----------------------------------------------------------------------------
;; Realtek 8812BU (external PA)default installation
;;----------------------------------------------------------------------------




[EXT_RTL8812bu.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, ePA_RTL8812bu.common.reg, VHT24G.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[EXT_RTL8812bu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[EXT_RTL8812bu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;----------------------------------------------------------------------------
;; LiteOn 8812BU default installation
;;----------------------------------------------------------------------------




[LITEON_RTL8812bu.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, LITEON_RTL8812bu.common.reg, VHT24G.reg,NdisSS.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[LITEON_RTL8812bu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[LITEON_RTL8812bu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration





;;----------------------------------------------------------------------------
;; Realtek 8821CU default installation
;;----------------------------------------------------------------------------




[RTL8821cu.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, RTL8821cu.common.reg, VHT24G.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8821cu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8821cu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;----------------------------------------------------------------------------
;; Realtek 8811CU default installation
;;----------------------------------------------------------------------------




[RTL8811cu.ndi.NT]
AddReg				= NDIS_63.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, RTL8811cu.common.reg, VHT24G.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8811cu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8811cu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;----------------------------------------------------------------------------
;;----------------------------------------------------------------------------




[RTL8723du.ndi.NT]
AddReg				= NDIS_63.reg, RTL8723du_common.reg, 11nWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, ConnectedStandbyEnable.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, BandWidthSetting.reg, NdisSS.reg, PnpPreTransOn.reg, LPSOn.reg, IPSOn.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8723du.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8723du.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;----------------------------------------------------------------------------
;;----------------------------------------------------------------------------




[RTL8710bu.ndi.NT]
AddReg				= NDIS_63.reg, RTL8710bu_common.reg, 11nWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, ConnectedStandbyEnable.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, BandWidthSetting.reg, NdisSS.reg, PnpPreTransOn.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8710bu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8710bu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;
;; OS relative registry.
;;
[NDIS_63.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5,mdcwifi"
HKR, Ndi\Interfaces,	LowerRange, 0, "wlan,ethernet,vwifi"
HKR, Ndi,				Service,    0, "RtlWlanu"
;;
;; OS relative service.
;;
[RtlWlanu.Service]
DisplayName    	= %RtlWlanu.DeviceDesc.DispName%
ServiceType    	= 1		; %SERVICE_KERNEL_DRIVER%
StartType      	= 3		; %SERRVICE_DEMAND_START%
ErrorControl   	= 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  	= %12%\rtwlanu.sys
LoadOrderGroup 	= NDIS

;;
;; OS relative event log.
;;
[RtlWlanu.EventLog]
AddReg 			= RtlWlanu.AddEventLog.reg

[RtlWlanu.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

[MCCDisable.reg]
HKR,Ndi\params\MultiChannelFcsMode, 		ParamDesc, 	0, "Multi-Channel Concurrent"
HKR,Ndi\params\MultiChannelFcsMode, 		type, 		0, "enum"
HKR,Ndi\params\MultiChannelFcsMode, 		default, 	0, "0"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"0", 		0, "Disabled"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"12", 		0, "Enabled"
HKR,defaults,MultiChannelFcsMode, 0, "0"
HKR,,MultiChannelFcsMode, 0, "0"

;*******************************************************************************
; USB common paramters
;*******************************************************************************
[UsbCommon.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"


;; For Different AC mode Rx parameters.
HKR,,AcUsbDmaTime,0,"10"
HKR,,AcUsbDmaSize,0,"5"
HKR,,AcUsbDmaTime2,0,"32"
HKR,,AcUsbDmaSize2,0,"5"


;; For Init mode
HKR,,FWOffload,0,"2"


;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;; For Hotspot UI Select Network Band
HKR,defaults,WdiGOon5GHzBandSupported,0,"0"
HKR,,WdiGOon5GHzBandSupported,0,"0"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation OS Relative
;-------------------------------------------------------------------------------

[Ndis6UsbRxAgg.reg]
HKR,defaults,UsbRxAggMode,0,"2"
HKR,,UsbRxAggMode,0,"2"
HKR,defaults,UsbRxAggPageCount,0,"16"
HKR,,UsbRxAggPageCount,0,"16"


[Ndis6UsbRxAgg_Jaguar.reg]
HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"
HKR,defaults,UsbRxAggPageCount,0,"5"
HKR,,UsbRxAggPageCount,0,"5"
HKR,defaults,UsbRxAggPageTimeout,0,"32"
HKR,,UsbRxAggPageTimeout,0,"32"


;;----------------------------------------------------------------------------
;; Wake on Wlan mode option parameters
;;----------------------------------------------------------------------------
[WowlanEnable.reg]
HKR,,WoWLANLPSLevel,0,"2"
HKR,,PingPatternEnable,0,"0"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

[WowlanDisable.reg]
HKR,,WoWLANLPSLevel,0,"0"
HKR,,PingPatternEnable,0,"0"

[WowlanAllEnableNoLPS.reg]
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"
HKR,,PingPatternEnable,0,"0"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

[WowlanAllEnablePingPatternNoLPS.reg]
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

HKR, Ndi\params\PingPatternEnable,         ParamDesc,  0, %PingPatternEnable%
HKR, Ndi\params\PingPatternEnable,         default,    0, "1"
HKR, Ndi\params\PingPatternEnable,         type,       0, "enum"
HKR, Ndi\params\PingPatternEnable\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\PingPatternEnable\enum,    "1",        0, %ENABLE_STR%

[WowlanEnableNoLPSNoPatternMatch.reg]
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"
HKR,,PingPatternEnable,0,"0"
HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "0"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

[ConnectedStandbyEnable.reg]
HKR,,WoWLANLPSLevel,0,"2"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"
HKR,,D2ListenIntvl,0,"4"
HKR,,NSOffloadEnable,0,"1"
HKR,,NLOEnable,0,"1"
HKR,,PingPatternEnable,0,"0"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "0"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

;; Packet coalescing should be enabled in WHCK test
HKR,defaults,*PacketCoalescing,0,"0"
HKR,,*PacketCoalescing,0,"0"

;-------------------------------------------------------------------------------
;	USB selective suspend.
;-------------------------------------------------------------------------------
[RtlSsOnn.reg]
HKR,,EnableUsbSS,0,"1"
[RtlSsOff.reg]
HKR,,EnableUsbSS,0,"0"

;-------------------------------------------------------------------------------
;	PnP pre-transition handling
;-------------------------------------------------------------------------------
[PnpPreTransOn.reg]
HKR,,PreTransPnP,0,"1"
[PnpPreTransOff.reg]
HKR,,PreTransPnP,0,"0"

;-------------------------------------------------------------------------------
;	TX path selection.
;-------------------------------------------------------------------------------
[TxByTimerOnn.reg]
HKR,,SendPacketByTimer,0,"1"
[TxByTimerOff.reg]
HKR,,SendPacketByTimer,0,"0"

;-------------------------------------------------------------------------------
;	TX power training disable.
;-------------------------------------------------------------------------------
[DisableTxPowerTraining.reg]
HKR,,TxPowerTraining,0,"0"


;-------------------------------------------------------------------------------
;	IPS selection.
;-------------------------------------------------------------------------------
[IPSOn.reg]
HKR,defaults,InactivePs,0,"2"
HKR,,InactivePs,0,"2"
[IPSOff.reg]
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

;-------------------------------------------------------------------------------
;	LPS selection.
;-------------------------------------------------------------------------------
[LPSOn.reg]
HKR,defaults,bLeisurePs,0,"1"
HKR,,bLeisurePs,0,"1"
[LPSOff.reg]
HKR,defaults,bLeisurePs,0,"0"
HKR,,bLeisurePs,0,"0"

;-------------------------------------------------------------------------------
;     Timer GPIO.
;-------------------------------------------------------------------------------
[TimerGPIOSetting8821AU.reg]
;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"2000"
HKR,,GPIOBack,0,"2000"

[TimerGPIOSetting8812AU.reg]
;; For GPIO detect setting.
HKR,,TimerGPIO,0,"1"
HKR,,GPIODelay,0,"500"
HKR,,GPIOBack,0,"250"

;---------------------------------------------------------------------------------
;    Customer ID
;---------------------------------------------------------------------------------
[CustomerID_Belkin.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"22"

[CustomerID_DLink.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"44"

[CustomerID_NEC.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"45"

[CustomerID_ASUS.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"35"

[CustomerLED8814A_TREND.reg]
; For Customer ID setting.
HKR,,LedStrategy, 0,"18"

;;----------------------------------------------------------------------------
;; TCP Reorder Control Parameters
;;----------------------------------------------------------------------------
[TcpReorderEnable.reg]
HKR,,TcpReorder,0,"1"
[TcpReorderDisable.reg]
HKR,,TcpReorder,0,"0"

;;----------------------------------------------------------------------------
;; Earlymode Control Parameters
;;----------------------------------------------------------------------------
[EarlyModeEnable.reg]
HKR,,bEarlymodeEnable,0,"1"
[EarlyModeDisable.reg]
HKR,,bEarlymodeEnable,0,"0"

;-------------------------------------------------------------------------------
;	Custom Tx Power Limit And Power By Rate Parameters
;-------------------------------------------------------------------------------
[CustomTxPwrConfigFile.reg]
HKR,,PwrByRateFile,0,""
HKR,,PwrLimitFile,0,""

;-------------------------------------------------------------------------------
; Intel Soft AP Mode Reg
;-------------------------------------------------------------------------------
[Intel.reg]
HKR,Ndi\params\ForcedBstDataRate,        ParamDesc,  0, "Broadcast/Multicast Data Rate"
HKR,Ndi\params\ForcedBstDataRate,        type,       0, "enum"
HKR,Ndi\params\ForcedBstDataRate,        default,    0, "0"
HKR,Ndi\params\ForcedBstDataRate\enum,   "0",        0, "Auto"
HKR,Ndi\params\ForcedBstDataRate\enum,   "2",        0, "1Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "4",        0, "2Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "11",      0, "5.5Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "22",     0, "11Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "12",      0, "6Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "18",     0, "9Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "24",     0, "12Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "36",     0, "18Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "48",     0, "24Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "72",     0, "36Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "96",     0, "48Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "108",     0, "54Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "128",     0, "MCS0"
HKR,Ndi\params\ForcedBstDataRate\enum,   "129",     0, "MCS1"
HKR,Ndi\params\ForcedBstDataRate\enum,   "130",     0, "MCS2"
HKR,Ndi\params\ForcedBstDataRate\enum,   "131",     0, "MCS3"
HKR,Ndi\params\ForcedBstDataRate\enum,   "132",     0, "MCS4"
HKR,Ndi\params\ForcedBstDataRate\enum,   "133",     0, "MCS5"
HKR,Ndi\params\ForcedBstDataRate\enum,   "134",     0, "MCS6"
HKR,Ndi\params\ForcedBstDataRate\enum,   "135",     0, "MCS7"
HKR,Ndi\params\ForcedBstDataRate\enum,   "136",     0, "MCS8"
HKR,Ndi\params\ForcedBstDataRate\enum,   "137",     0, "MCS9"
HKR,Ndi\params\ForcedBstDataRate\enum,   "138",     0, "MCS10"
HKR,Ndi\params\ForcedBstDataRate\enum,   "139",     0, "MCS11"
HKR,Ndi\params\ForcedBstDataRate\enum,   "140",     0, "MCS12"
HKR,Ndi\params\ForcedBstDataRate\enum,   "141",     0, "MCS13"
HKR,Ndi\params\ForcedBstDataRate\enum,   "142",     0, "MCS14"
HKR,Ndi\params\ForcedBstDataRate\enum,   "143",     0, "MCS15"


;*******************************************************************************
; RTL8723au common paramters
;*******************************************************************************
[RTL8723_common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;*******************************************************************************
; RTL8723du common paramters
;*******************************************************************************
[RTL8723du_common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"

;; For LDPC Cap
HKR,defaults,LdpcCap,0,"0"

;; For STBC Cap
HKR,defaults,StbcCap,0,"16" 
;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"


;*******************************************************************************
; RTL8710bu common paramters
;*******************************************************************************
[RTL8710bu_common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"

;; For LDPC Cap
HKR,defaults,LdpcCap,0,"0"

;; For STBC Cap
HKR,defaults,StbcCap,0,"16" 

;; For Address offset of Page 0
HKR,defaults,Page0Offset,0,"32768"
HKR,,Page0Offset,0,"32768" 
;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"


;*******************************************************************************
; RTL8723bu common paramters
;*******************************************************************************
[RTL8723b_common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"
;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;*******************************************************************************
; RTL8188fu common paramters
;*******************************************************************************
[RTL8188fu.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;*******************************************************************************
; RTL8188eu common paramters
;*******************************************************************************
[RTL8188eu.common.reg]
;; For SoftApBss creator side judgement.
 

;*******************************************************************************
; RTL8812au common paramters
;*******************************************************************************
[RTL8812au.common.reg]
;; For IQK Offload to FW.
HKR,,IQKFWOffload,0,"1"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,AggDMEnable,0,"1"
HKR,,AggDMEnable,0,"1"

;; Prefer Band
HKR,Ndi\params\PreferBand, 			ParamDesc, 	0, "Preferred Band"
HKR,Ndi\params\PreferBand, 			default, 	0, "0"
HKR,Ndi\params\PreferBand, 			type, 		0, "enum"
HKR,Ndi\params\PreferBand\enum, 	"0", 		0, "1. No Preference"
HKR,Ndi\params\PreferBand\enum, 	"1", 		0, "2. 2.4G first"
HKR,Ndi\params\PreferBand\enum, 	"2", 		0, "3. 5G first"
HKR,,PreferBand,0,"0"

;; 8812AU support VHT24G mode.
HKR,Ndi\params\Vht24g, 		ParamDesc, 	0, "VHT 2.4G IOT"
HKR,Ndi\params\Vht24g, 		type, 		0, "enum"
HKR,Ndi\params\Vht24g, 		default, 	0, "255"
HKR,Ndi\params\Vht24g\enum, 	"0", 	0, "Disable"
HKR,Ndi\params\Vht24g\enum, 	"255", 	0, "Enable"
HKR,Ndi\params\Vht24g\enum, 	"254", 	0, "Not support Broadcom vendor"
HKR,defaults,Vht24g, 0, "255"
HKR,,Vht24g, 0, "255"

HKR,defaults,AddbaReqRetry,0,"0"
HKR,,AddbaReqRetry,0,"0"

;*******************************************************************************
; RTL8814au common paramters
;*******************************************************************************
[RTL8814au.common.reg]
HKR,,UsbRxAggMode,0,"1"
HKR,,IQKFWOffload,0,"0"
HKR,,UsbTxAggTotalNum,0,"24"
HKR,,UsbTxAggDescNum,0,"3"

HKR,,FWOffload,0,"2"
HKR,,ValidRFPath,0,"239"
HKR,,PreInitMem,0,"1"

HKR,defaults,AggDMEnable,0,"1"
HKR,,AggDMEnable,0,"1"
HKR,,RxReorder_FlushChk,0,"1"

;; Enable AMSDU of AMPDU.
HKR,Ndi\params\AMfactor,        ParamDesc,  0, "AMfactor"
HKR,Ndi\params\AMfactor,        type,       0, "enum"
HKR,Ndi\params\AMfactor,        default,    0, "7"
HKR,Ndi\params\AMfactor\enum,   "7",        0, "VHT AMPDU"
HKR,Ndi\params\AMfactor\enum,   "252",      0, "VHT AMSDU in AMPDU Mode 1"
HKR,Ndi\params\AMfactor\enum,   "253",      0, "VHT AMSDU in AMPDU Mode 2"
;;HKR,Ndi\params\AMfactor\enum,   "254",        0, "VHT LDPC TX"
HKR,Ndi\params\AMfactor\enum,   "251",      0, "VHT AMSDU in AMPDU Mode Manual"
HKR,defaults,AMfactor,0,"253"
HKR,,AMfactor,0,"253"
HKR,,AMfactor,,"253"

;; STBC 
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "17",        0, "HT/VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "34",        0, "HT/VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;; LDPC 
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "17",        0, "HT/VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "34",        0, "HT/VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"

;; BEAMFORMING
HKR,Ndi\params\BeamformCap,        ParamDesc,  0, "BeamCap"
HKR,Ndi\params\BeamformCap,        type,       0, "enum"
HKR,Ndi\params\BeamformCap,        default,    0, "0"
HKR,Ndi\params\BeamformCap\enum,   "0",        0, "BEAM Disable"
HKR,Ndi\params\BeamformCap\enum,   "3",        0, "VHT BEAM TX|RX"
HKR,Ndi\params\BeamformCap\enum,   "17",        0, "HT/VHT BEAM TX"
HKR,Ndi\params\BeamformCap\enum,   "34",        0, "HT/VHT BEAM RX"
HKR,Ndi\params\BeamformCap\enum,   "51",       0, "VHT BEAM TX|RX & HT BEAM TX|RX"
HKR,defaults,BeamformCap,0,"51"
HKR,,BeamformCap,0,"51"
HKR,,BeamformCap,,"51"

;; USB Switch Fast Mode
HKR,Ndi\params\UsbSwFast, 	ParamDesc, 	0, "USB SF Mode"
HKR,Ndi\params\UsbSwFast, 	type, 		0, "enum"
HKR,Ndi\params\UsbSwFast, 	default, 	0, "1"
HKR,Ndi\params\UsbSwFast\enum, 	"0", 	0, "Disable"
HKR,Ndi\params\UsbSwFast\enum, 	"1", 	0, "Enable"
HKR,defaults,UsbSwFast,0,"1"
HKR,,UsbSwFast,0,"1"

;; USB Device/Host Control RF Path
HKR,Ndi\params\UsbRfSet, 	ParamDesc, 	0, "USB RF SELECT"
HKR,Ndi\params\UsbRfSet, 	type, 		0, "enum"
HKR,Ndi\params\UsbRfSet, 	default, 	0, "0"
HKR,Ndi\params\UsbRfSet\enum, 	"0", 	0, "BY DEV/HOST"
HKR,Ndi\params\UsbRfSet\enum, 	"1", 	0, "HW DEFAULT SET"
HKR,defaults,UsbRfSet,0,"0"
HKR,,UsbRfSet,0,"0"


;*******************************************************************************
; RTL8814au common paramters 3T3R
;*******************************************************************************
[RTL8814au3T3R.common.reg]
HKR,,UsbRxAggMode,0,"1"
HKR,,IQKFWOffload,0,"0"
HKR,,UsbTxAggTotalNum,0,"24"
HKR,,UsbTxAggDescNum,0,"3"

HKR,,FWOffload,0,"2"
HKR,,ValidRFPath,0,"238"
HKR,,PreInitMem,0,"1"

;; Enable AMSDU of AMPDU.
HKR,Ndi\params\AMfactor,        ParamDesc,  0, "AMfactor"
HKR,Ndi\params\AMfactor,        type,       0, "enum"
HKR,Ndi\params\AMfactor,        default,    0, "7"
HKR,Ndi\params\AMfactor\enum,   "7",        0, "VHT AMPDU"
HKR,Ndi\params\AMfactor\enum,   "252",      0, "VHT AMSDU in AMPDU Mode 1"
HKR,Ndi\params\AMfactor\enum,   "253",      0, "VHT AMSDU in AMPDU Mode 2"
;;HKR,Ndi\params\AMfactor\enum,   "254",        0, "VHT LDPC TX"
HKR,Ndi\params\AMfactor\enum,   "251",      0, "VHT AMSDU in AMPDU Mode Manual"
HKR,defaults,AMfactor,0,"253"
HKR,,AMfactor,0,"253"
HKR,,AMfactor,,"253"

;; STBC 
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "17",        0, "HT/VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "34",        0, "HT/VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;; LDPC 
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "17",        0, "HT/VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "34",        0, "HT/VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"

;; BEAMFORMING
HKR,Ndi\params\BeamformCap,        ParamDesc,  0, "BeamCap"
HKR,Ndi\params\BeamformCap,        type,       0, "enum"
HKR,Ndi\params\BeamformCap,        default,    0, "0"
HKR,Ndi\params\BeamformCap\enum,   "0",        0, "BEAM Disable"
HKR,Ndi\params\BeamformCap\enum,   "3",        0, "VHT BEAM TX|RX"
HKR,Ndi\params\BeamformCap\enum,   "17",        0, "HT/VHT BEAM TX"
HKR,Ndi\params\BeamformCap\enum,   "34",        0, "HT/VHT BEAM RX"
HKR,Ndi\params\BeamformCap\enum,   "51",       0, "VHT BEAM TX|RX & HT BEAM TX|RX"
HKR,defaults,BeamformCap,0,"51"
HKR,,BeamformCap,0,"51"
HKR,,BeamformCap,,"51"

;; USB Switch Fast Mode
HKR,Ndi\params\UsbSwFast, 	ParamDesc, 	0, "USB SF Mode"
HKR,Ndi\params\UsbSwFast, 	type, 		0, "enum"
HKR,Ndi\params\UsbSwFast, 	default, 	0, "1"
HKR,Ndi\params\UsbSwFast\enum, 	"0", 	0, "Disable"
HKR,Ndi\params\UsbSwFast\enum, 	"1", 	0, "Enable"
HKR,defaults,UsbSwFast,0,"1"
HKR,,UsbSwFast,0,"1"

;; USB Device/Host Control RF Path
HKR,Ndi\params\UsbRfSet, 	ParamDesc, 	0, "USB RF SELECT"
HKR,Ndi\params\UsbRfSet, 	type, 		0, "enum"
HKR,Ndi\params\UsbRfSet, 	default, 	0, "0"
HKR,Ndi\params\UsbRfSet\enum, 	"0", 	0, "BY DEV/HOST"
HKR,Ndi\params\UsbRfSet\enum, 	"1", 	0, "HW DEFAULT SET"
HKR,defaults,UsbRfSet,0,"0"
HKR,,UsbRfSet,0,"0"



;*******************************************************************************
; RTL8822bu common paramters
;*******************************************************************************
[RTL8822bu.common.reg]
HKR,,UsbRxAggMode,0,"3"
HKR,,IQKFWOffload,0,"0"
HKR,,BeamformCap,0,"42"
HKR,,ValidRFPath,0,"51"
HKR,,PreInitMem,0,"1"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,RFEType,0,"3"
HKR,,ForcedUsbMode,0,"1"
HKR,,AMfactor,0,"253"
HKR,,RxReorder,0,"1"
HKR,,LinkSpeedLevel,0,"18"
HKR,,ECSSupport,0,"0"

;; STBC 
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "17",        0, "HT/VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "34",        0, "HT/VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;; LDPC 
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "17",        0, "HT/VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "34",        0, "HT/VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"

;*******************************************************************************
; RTL8812bu (iPA)common paramters
;*******************************************************************************
[RTL8812bu.common.reg]
HKR,,UsbRxAggMode,0,"3"
HKR,,IQKFWOffload,0,"0"
HKR,,BeamformCap,0,"42"
HKR,,ValidRFPath,0,"51"
HKR,,PreInitMem,0,"1"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,RFEType,0,"3"
HKR,,AMfactor,0,"253"
HKR,,ForcedUsbMode,0,"0"
HKR,,RxReorder,0,"1"
HKR,,LinkSpeedLevel,0,"18"

HKR,,ECSSupport,0,"0"

;; STBC 
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "17",        0, "HT/VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "34",        0, "HT/VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;; LDPC 
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "17",        0, "HT/VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "34",        0, "HT/VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"

;*******************************************************************************
; RTL8812bu (iPA force U2)common paramters
;*******************************************************************************
[U2_RTL8812bu.common.reg]
HKR,,UsbRxAggMode,0,"3"
HKR,,IQKFWOffload,0,"0"
HKR,,BeamformCap,0,"42"
HKR,,ValidRFPath,0,"51"
HKR,,PreInitMem,0,"1"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,RFEType,0,"3"
HKR,,ForcedUsbMode,0,"1"
HKR,,AMfactor,0,"253"
HKR,,LinkSpeedLevel,0,"18"
HKR,,RxReorder,0,"1"

HKR,,ECSSupport,0,"0"

;; STBC 
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "17",        0, "HT/VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "34",        0, "HT/VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;; LDPC 
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "17",        0, "HT/VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "34",        0, "HT/VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"
;*******************************************************************************
; RTL8812bu (ePA)common paramters
;*******************************************************************************
[ePA_RTL8812bu.common.reg]
HKR,,UsbRxAggMode,0,"3"
HKR,,IQKFWOffload,0,"0"
HKR,,BeamformCap,0,"42"
HKR,,ValidRFPath,0,"51"
HKR,,PreInitMem,0,"1"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,RFEType,0,"2"
HKR,,LinkSpeedLevel,0,"18"
HKR,,AMfactor,0,"253"
HKR,,ForcedUsbMode,0,"0"
HKR,,RxReorder,0,"1"

HKR,,ECSSupport,0,"0"

;; STBC 
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "17",        0, "HT/VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "34",        0, "HT/VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;; LDPC 
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "17",        0, "HT/VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "34",        0, "HT/VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"

[Belkin_RTL8812bu.common.reg]
HKR,,UsbRxAggMode,0,"3"
HKR,,IQKFWOffload,0,"0"
HKR,,BeamformCap,0,"42"
HKR,,ValidRFPath,0,"51"
HKR,,PreInitMem,0,"1"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,RFEType,0,"3"
HKR,,AMfactor,0,"253"
HKR,,ForcedUsbMode,0,"0"
HKR,,RegROAMSensitiveLevel,0,"70"
HKR,,LinkSpeedLevel,0,"18"
HKR,,RxReorder,0,"1"

HKR,,ECSSupport,0,"0"

;; STBC 
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "17",        0, "HT/VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "34",        0, "HT/VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;; LDPC 
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "17",        0, "HT/VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "34",        0, "HT/VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"
[8812BUOffloadCap.reg]
HKR,,MacSupportAbility,0,"2155413565"

;*******************************************************************************
; LiteOn 8812bu  common paramters
;*******************************************************************************
[LITEON_RTL8812bu.common.reg]
HKR,,UsbRxAggMode,0,"3"
HKR,,IQKFWOffload,0,"0"
HKR,,BeamformCap,0,"42"
HKR,,ValidRFPath,0,"51"
HKR,,PreInitMem,0,"1"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,RFEType,0,"3"
HKR,,AMfactor,0,"253"
HKR,,ForcedUsbMode,0,"0"
HKR,,RxReorder,0,"1"
HKR,,LinkSpeedLevel,0,"18"
HKR,,InactivePs,0,"1"
HKR,,ECSSupport,0,"0"

;; STBC 
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "17",        0, "HT/VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "34",        0, "HT/VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;; LDPC 
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "17",        0, "HT/VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "34",        0, "HT/VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"


;*******************************************************************************
; RTL8821cu common paramters
;*******************************************************************************
[RTL8821cu.common.reg]
HKR,,UsbRxAggMode,0,"3"
HKR,,IQKFWOffload,0,"0"
HKR,,BeamformCap,0,"42"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,ValidRFPath,0,"17"
HKR,,PreInitMem,0,"1"
HKR,,RxReorder,0,"1"
;; STBC 
HKR,,StbcCap,0,"0"
;; LDPC 
HKR,,LdpcCap,0,"34"

;*******************************************************************************
; RTL8811cu common paramters
;*******************************************************************************
[RTL8811cu.common.reg]
HKR,,UsbRxAggMode,0,"3"
HKR,,IQKFWOffload,0,"0"
HKR,,BeamformCap,0,"42"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,ValidRFPath,0,"17"
HKR,,PreInitMem,0,"1"
;; STBC 
HKR,,StbcCap,0,"0"
;; LDPC 
HKR,,LdpcCap,0,"34"

;;----------------------------------------------------------------------------
;; LDPC config parameters 8812/8814 only now! Other IC need to assign another value.
;;----------------------------------------------------------------------------

[LDPC_CONFIG.reg]
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "34"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "1",        0, "VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "2",        0, "VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "34",        0, "VHT LDPC TX | HT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"34"
HKR,,LdpcCap,0,"34"
HKR,,LdpcCap,,"34"

;;----------------------------------------------------------------------------
;; STBC config parameters 8812/8814 only now! Other IC need to assign another value.
;;----------------------------------------------------------------------------

[STBC_CONFIG.reg]
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "1",        0, "VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "2",        0, "VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;;----------------------------------------------------------------------------
;; Beamformer config parameters 8812/8814 only now! Other IC need to assign another value.
;;----------------------------------------------------------------------------

[BEAM_CONFIG.reg]
HKR,Ndi\params\BeamformCap,        ParamDesc,  0, "BeamCap"
HKR,Ndi\params\BeamformCap,        type,       0, "enum"
HKR,Ndi\params\BeamformCap,        default,    0, "51"
HKR,Ndi\params\BeamformCap\enum,   "0",        0, "BEAM Disable"
HKR,Ndi\params\BeamformCap\enum,   "3",        0, "VHT BEAM TX|RX"
HKR,Ndi\params\BeamformCap\enum,   "1",        0, "VHT BEAM TX"
HKR,Ndi\params\BeamformCap\enum,   "2",        0, "VHT BEAM RX"
HKR,Ndi\params\BeamformCap\enum,   "51",       0, "VHT BEAM TX|RX & HT BEAM TX|RX"
HKR,defaults,BeamformCap,0,"34"
HKR,,BeamformCap,0,"34"
HKR,,BeamformCap,,"34"

;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,defaults,bNewRcvRefCnt,0,"1"
HKR,,bNewRcvRefCnt,0,"1"

HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

HKR,defaults,StaUapsd,0,"0"
HKR,,StaUapsd,0,"0"

;;Tx power limit
HKR,,EnableTxPowerLimit,0,"2"

;; For QoS test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\QoS,        ParamDesc,  0, "QoS Support"
HKR,Ndi\params\QoS,        type,       0, "enum"
HKR,Ndi\params\QoS,        default,    0, "0"
HKR,Ndi\params\QoS\enum,   "0",        0, "Not Support QoS"
HKR,Ndi\params\QoS\enum,   "1",        0, "Support QoS"
HKR,Ndi\params\QoS\enum,   "2",        0, "Auto"
HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"
HKR,,QoS,,"1"


HKR,defaults,RxReorder,0,"1"
HKR,,RxReorder,0,"1"
HKR,defaults,RegRxReorder_WinSize,0,"128"
HKR,,RegRxReorder_WinSize,0,"128"
HKR,defaults,RxReorder_PendTime,0,"100"
HKR,,RxReorder_PendTime,0,"100"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"0"
HKR,,bLeisurePs,0,"0"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"1"
HKR,,bFwCtrlLPS,0,"1"

;; LPS Interval
HKR,,LPSIntvl,0,"5"

;BTmode
HKR,,bBTMode,0,"1"

; Reset Tx Hang
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"

HKR,,WEPinNmode,0,"0"

; OS protocol offload detection and decision
HKR,,ProtocolOffloadDecision,0,"1"

; Win8 FSS mode detection mechanism
HKR,,FSSDetection,0,"0"

HKR,defaults,AddbaReqRetry,0,"0"
HKR,,AddbaReqRetry,0,"0"

;;Define enable status of each RT Bug Check IDs
HKR,,BugCheckIdLogEnConfig,0x10001,0x7FFF


;-------------------------------------------------------------------------------
;	Some function ability setting
;-------------------------------------------------------------------------------
HKR,defaults,LinkSpeedLevel,0,"0"
HKR,,LinkSpeedLevel,0,"0"

HKR,defaults,TxMode,0,"0"
HKR,,TxMode,0,"0"

HKR,defaults,PwrTblSel,0,"0"
HKR,,PwrTblSel,0,"0"

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"

HKR,defaults,PHYParaFromFolder,0,"0"
HKR,,PHYParaFromFolder,0,"0"

;Dynamic batch indication
HKR,defaults,DynamicBatchEnable,0,"1"
HKR,,DynamicBatchEnable,0,"1"

HKR,defaults,BINumber,0,"10"
HKR,,BINumber,0,"10"

HKR,Ndi\params\EnableAdaptivity, 		ParamDesc, 	0, "EnableAdaptivity"
HKR,Ndi\params\EnableAdaptivity, 		type, 		0, "enum"
HKR,Ndi\params\EnableAdaptivity, 		default, 	0, "0"
HKR,Ndi\params\EnableAdaptivity\enum, 	"0", 		0, "Disable"
HKR,Ndi\params\EnableAdaptivity\enum, 	"1", 		0, "Enable"
HKR,Ndi\params\EnableAdaptivity\enum, 	"2", 		0, "Auto"
HKR,defaults,EnableAdaptivity, 0, "2"
HKR,,EnableAdaptivity, 0, "2"

HKR,Ndi\params\L2HForAdaptivity, 		ParamDesc, 	0, "L2HForAdaptivity"
HKR,Ndi\params\L2HForAdaptivity, 		type, 		0, "enum"
HKR,Ndi\params\L2HForAdaptivity, 		default, 	0, "Auto"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"0", 		0, "Auto"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"245", 		0, "F5"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"243", 		0, "F3"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"241", 		0, "F1"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"239", 		0, "EF"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"237", 		0, "ED"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"235", 		0, "EB"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"232", 		0, "E8"
HKR,defaults,L2HForAdaptivity, 0, "0"
HKR,,L2HForAdaptivity, 0, "0"

HKR,Ndi\params\HLDiffForAdaptivity, 		ParamDesc, 	0, "HLDiffForAdaptivity"
HKR,Ndi\params\HLDiffForAdaptivity, 		type, 		0, "enum"
HKR,Ndi\params\HLDiffForAdaptivity, 		default, 	0, "7"
HKR,Ndi\params\HLDiffForAdaptivity\enum, 	"7", 		0, "7"
HKR,Ndi\params\HLDiffForAdaptivity\enum, 	"9", 		0, "9"
HKR,defaults,HLDiffForAdaptivity, 0, "7"
HKR,,HLDiffForAdaptivity, 0, "7"

HKR,Ndi\params\AdaptivityPara, 		ParamDesc, 	0, "AdaptivityPara"
HKR,Ndi\params\AdaptivityPara, 		type, 		0, "enum"
HKR,Ndi\params\AdaptivityPara, 		default, 	0, "0"
HKR,Ndi\params\AdaptivityPara\enum, 	"0", 		0, "0"
HKR,Ndi\params\AdaptivityPara\enum, 	"1", 		0, "1"
HKR,defaults,AdaptivityPara, 0, "0"
HKR,,AdaptivityPara, 0, "0"

; TPC mechenisum
; HKR,Ndi\params\TPCEnable,        ParamDesc,  0, "TPCEnable"
; HKR,Ndi\params\TPCEnable,        type,       0, "enum"
; HKR,Ndi\params\TPCEnable,        default,    0, "0"
; HKR,Ndi\params\TPCEnable\enum,   "0",        0, "TPC Disable"
; HKR,Ndi\params\TPCEnable\enum,   "1",        0, "ETSI Enable"
; HKR,Ndi\params\TPCEnable\enum,   "2",        0, "MKK Enable"
; HKR,Ndi\params\TPCEnable\enum,   "4",        0, "FCC Enable"
; HKR,Ndi\params\TPCEnable\enum,   "8",        0, "WW Enable"
; HKR,Ndi\params\TPCEnable\enum,   "15",        0, "Enable All"
; HKR,defaults,TPCEnable,0,"0"
; HKR,,TPCEnable,0,"0"

; HKR,Ndi\params\TxPowerControl,        ParamDesc,  0, "TxPowerControl"
; HKR,Ndi\params\TxPowerControl,        type,       0, "enum"
; HKR,Ndi\params\TxPowerControl,        default,    0, "0"
; HKR,Ndi\params\TxPowerControl\enum,   "0",        0, "100%"
; HKR,Ndi\params\TxPowerControl\enum,   "1",        0, "50%"
; HKR,Ndi\params\TxPowerControl\enum,   "2",        0, "0"
; HKR,defaults,TxPowerControl,0,"0"
; HKR,,TxPowerControl,0,"0"


[Ndis5Set.reg]
HKR,Ndi\params\PSPXlinkMode,			ParamDesc,  0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode,			type,       0, "enum"
HKR,Ndi\params\PSPXlinkMode,			default,    0, "0"
HKR,Ndi\params\PSPXlinkMode\enum,		"0",        0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum,		"1",        0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"

;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

HKR,defaults,AggDMEnable,0,"0"
HKR,,AggDMEnable,0,"0"

[Ndis6Set.reg]
;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"


;;----------------------------------------------------------------------------
;; Win7 high throughput(8814) Rxreorder setting
;;----------------------------------------------------------------------------
[N61RxReorder.reg]
HKR,defaults,RegRxReorder_WinSize,0,"64"
HKR,,RegRxReorder_WinSize,0,"64"
HKR,defaults,RxReorder_PendTime,0,"30"
HKR,,RxReorder_PendTime,0,"30"


[NEC.reg]
HKR,Ndi\params\TxPwrPercentage, 	ParamDesc, 	0, %TX_PWR_CONTROL_STR%
HKR,Ndi\params\TxPwrPercentage, 	type, 		0, "enum"
HKR,Ndi\params\TxPwrPercentage, 	default, 	0, "8"
HKR,Ndi\params\TxPwrPercentage\enum, 	"1", 		0, %TX_PWR_PERCENTAGE_1_STR%
HKR,Ndi\params\TxPwrPercentage\enum, 	"2", 		0, %TX_PWR_PERCENTAGE_2_STR%
HKR,Ndi\params\TxPwrPercentage\enum, 	"4", 		0, %TX_PWR_PERCENTAGE_3_STR%
HKR,Ndi\params\TxPwrPercentage\enum, 	"8", 		0, %TX_PWR_PERCENTAGE_4_STR%
HKR,defaults,TxPwrPercentage, 0, "8"
HKR,,TxPwrPercentage, 0, "8"

HKR,Ndi\params\StreamMode, 	ParamDesc, 	0, %STREAM_MODE_STR%
HKR,Ndi\params\StreamMode, 	type, 		0, "enum"
HKR,Ndi\params\StreamMode, 	default, 	0, "0"
HKR,Ndi\params\StreamMode\enum, 	"0", 		0, "OFF"
HKR,Ndi\params\StreamMode\enum, 	"1", 		0, "ON"
HKR,defaults,StreamMode, 0, "0"
HKR,,StreamMode, 0, "0"

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"0"
HKR,,bLeisurePs,0,"0"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"1"
HKR,,bFwCtrlLPS,0,"1"

;; LPS Interval
;HKR,defaults,LPSIntvl,0,"5"
HKR,,LPSIntvl,0,"5"

;BTmode
HKR,,bBTMode,0,"1"

; Reset Tx Hang
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"

; OS protocol offload detection and decision
HKR,,ProtocolOffloadDecision,0,"1"

; Win8 FSS mode detection mechanism
HKR,,FSSDetection,0,"0"

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"

; /****************************************************************************
; ** Customerize Registry Area.
; ****************************************************************************/
[USBSwitch.reg]
HKR,Ndi\params\ForcedUsbMode, 	ParamDesc, 	0, "USB Switch Mode"
HKR,Ndi\params\ForcedUsbMode, 	type, 		0, "enum"
HKR,Ndi\params\ForcedUsbMode, 	default, 	0, "0"
HKR,Ndi\params\ForcedUsbMode\enum, 	"0", 	0, "Auto"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"1", 	0, "USB 2.0"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"2", 	0, "USB 3.0"
HKR,Ndi\params\ForcedUsbMode\enum, 	"3", 	0, "USB Mode 1"
HKR,Ndi\params\ForcedUsbMode\enum, 	"4", 	0, "USB Mode 2"
HKR,Ndi\params\ForcedUsbMode\enum, 	"8", 	0, "USB Mode 3"
HKR,defaults,ForcedUsbMode, 0, "0"
HKR,,ForcedUsbMode, 0, "0"

HKR,Ndi\params\UsbSwFast, 	ParamDesc, 	0, "USB SF Mode"
HKR,Ndi\params\UsbSwFast, 	type, 		0, "enum"
HKR,Ndi\params\UsbSwFast, 	default, 	0, "0"
HKR,Ndi\params\UsbSwFast\enum, 	"0", 	0, "Disable"
HKR,Ndi\params\UsbSwFast\enum, 	"1", 	0, "Enable"
HKR,defaults,UsbSwFast,0,"0"
HKR,,UsbSwFast,0,"0"

HKR,defaults,UsbSwitchSpeed,0,"10"
HKR,,UsbSwitchSpeed,0,"10"

HKR,defaults,UsbSwitchThL,0,"35"
HKR,,UsbSwitchThL,0,"35"

HKR,defaults,UsbSwitchThH,0,"45"
HKR,,UsbSwitchThH,0,"45"

HKR,defaults,UsbSwitchThRssi,0,"40"
HKR,,UsbSwitchThRssi,0,"40"


[USBSwitch3.reg]
HKR,Ndi\params\ForcedUsbMode, 	ParamDesc, 	0, "USB Switch Mode"
HKR,Ndi\params\ForcedUsbMode, 	type, 		0, "enum"
HKR,Ndi\params\ForcedUsbMode, 	default, 	0, "0"
HKR,Ndi\params\ForcedUsbMode\enum, 	"0", 	0, "Auto"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"1", 	0, "USB 2.0"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"2", 	0, "USB 3.0"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"3", 	0, "USB Mode 1"
HKR,Ndi\params\ForcedUsbMode\enum, 	"4", 	0, "USB Mode 2"
HKR,Ndi\params\ForcedUsbMode\enum, 	"8", 	0, "USB Mode 3"
HKR,defaults,ForcedUsbMode, 0, "8"
HKR,,ForcedUsbMode, 0, "8"

HKR,Ndi\params\UsbSwFast, 	ParamDesc, 	0, "USB SF Mode"
HKR,Ndi\params\UsbSwFast, 	type, 		0, "enum"
HKR,Ndi\params\UsbSwFast, 	default, 	0, "0"
HKR,Ndi\params\UsbSwFast\enum, 	"0", 	0, "Disable"
HKR,Ndi\params\UsbSwFast\enum, 	"1", 	0, "Enable"
HKR,defaults,UsbSwFast,0,"0"
HKR,,UsbSwFast,0,"0"

HKR,defaults,UsbSwitchSpeed,0,"50"
HKR,,UsbSwitchSpeed,0,"50"

HKR,defaults,UsbSwitchThL,0,"20"
HKR,,UsbSwitchThL,0,"20"

HKR,defaults,UsbSwitchThH,0,"5"
HKR,,UsbSwitchThH,0,"5"

HKR,defaults,UsbSwitchThRssi,0,"35"
HKR,,UsbSwitchThRssi,0,"35"


[USBModeVx.reg]
HKR,defaults,ForcedUsbMode, 0, "5"
HKR,,ForcedUsbMode, 0, "5"
 
[USBMode2.reg]
HKR,defaults,ForcedUsbMode, 0, "1"
HKR,,ForcedUsbMode, 0, "1"

[Signal.reg]
HKR,defaults,LinkSpeedLevel, 0, "28"
HKR,,LinkSpeedLevel, 0, "28"

[BeautifySignal.reg]
HKR,Ndi\params\LinkSpeedLevel, 	ParamDesc, 	0, "Beautify Signal Strength Level"
HKR,Ndi\params\LinkSpeedLevel, 	type, 		0, "enum"
HKR,Ndi\params\LinkSpeedLevel, 	default, 	0, "0"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"0", 	0, "Default"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"52", 	0, "SS Display Lvl1"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"54", 	0, "SS Display Lvl2"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"56", 	0, "SS Display Lvl3"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"58", 	0, "SS Display Lvl4"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"60", 	0, "SS Display Lvl5"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"62", 	0, "SS Display Lvl6"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"64", 	0, "SS Display Lvl7"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"68", 	0, "SS Display Lvl8"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"70", 	0, "SS Display Lvl9"
HKR,defaults,LinkSpeedLevel, 0, "0"
HKR,,LinkSpeedLevel, 0, "0"


[sifs.reg]
HKR,defaults,SifsThresh, 0, "0"
HKR,,SifsThresh, 0, "0"


[ScanType.reg]
HKR,defaults,PassiveScan, 0, "0"
HKR,,PassiveScan, 0, "0"

; /****************************************************************************
; ** IHV Service Reg for CCX
; ****************************************************************************/
[CIHVS.reg]
HKR, Ndi\IHVExtensions, ExtensibilityDLL,       0,  "%%SystemRoot%%\system32\Rtlihvs.dll"
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID,   0,  "{6C2A8CCA-B2A2-4d81-A3B2-4E15F445C312}"
HKR, Ndi\IHVExtensions, GroupName,              0,  "Realtek CCX SDK IHV Service"
HKR, Ndi\IHVExtensions, AdapterOUI,             0x00010001, 0x00e04c

;*******************************************************************************
; WAPI section
;*******************************************************************************
[wapi.reg]
HKR,defaults,WapiSupport,0,"1"
HKR,,WapiSupport,0,"1"


;;----------------------------------------------------------------------------
;; Belkin WLAN NIC parameters
;;----------------------------------------------------------------------------
[Belkin.reg]
HKR,Ndi\params\RFOff,			ParamDesc,  0, "Radio"
HKR,Ndi\params\RFOff,			type,       0, "enum"
HKR,Ndi\params\RFOff,			default,    0, "0"
HKR,Ndi\params\RFOff\enum,		"0",        0, "On"
HKR,Ndi\params\RFOff\enum,		"1",        0, "Off"
HKR,defaults,RFOff,0,"0"
HKR,,RFOff,0,"0"

;;----------------------------------------------------------------------------
;; Wireless Mode Related Parameters
;;----------------------------------------------------------------------------
[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

;; 40MHz Support in 11n
HKR,Ndi\params\BWSetting,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BWSetting,        type,       0, "enum"
HKR,Ndi\params\BWSetting,        default,    0, "1"
HKR,Ndi\params\BWSetting\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum,   "1",        0, "20_40MHz"
HKR,,BWSetting,0,"1"

HKR,,Channel,0,"10"

[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

HKR,,BWSetting,0,"0"

HKR,,Channel,0,"10"

[11agnWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %AUTO_STR%
HKR,Ndi\params\WirelessMode\enum, 	"1", 		0, %IEEE_802_11A_STR%
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"16", 		0, %IEEE_802_11BGN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"32", 		0, %IEEE_802_11AN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

[11acWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %AUTO_STR%
HKR,Ndi\params\WirelessMode\enum, 	"1", 		0, %IEEE_802_11A_STR%
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"16", 		0, %IEEE_802_11BGN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"32", 		0, %IEEE_802_11AN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"64", 		0, %IEEE_802_11ANAC_STR%
HKR,Ndi\params\WirelessMode\enum, 	"256", 		0, %IEEE_802_11AC_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

HKR,,Channel,0,"10"
HKR,,RFType,0,"15"

HKR,,BWSetting,0,"2"

[5G11acWirelessMode.reg]
HKR,,WirelessMode, 0, "64"
HKR,,Channel,0,"36"
HKR,,RFType,0,"15"
HKR,,BWSetting,0,"2"

;;----------------------------------------------------------------------------
;; 11AC series IC VHT 2.4G Support
;;----------------------------------------------------------------------------
[VHT24G.reg]
HKR,Ndi\params\Vht24g, 		ParamDesc, 	0, "VHT 2.4G"
HKR,Ndi\params\Vht24g, 		type, 		0, "enum"
HKR,Ndi\params\Vht24g, 		default, 	0, "255"
HKR,Ndi\params\Vht24g\enum, 	"0", 		0, "Disable"
HKR,Ndi\params\Vht24g\enum, 	"255", 		0, "Enable"
HKR,Ndi\params\Vht24g\enum, 	"254", 		0, "Not support Broadcom vendor"
HKR,defaults,Vht24g, 0, "255"
HKR,,Vht24g, 0, "255"

;;----------------------------------------------------------------------------
;; 11N or higher Adhoc Mode
;;----------------------------------------------------------------------------
[HAdhoc.reg]
HKR,Ndi\params\11nAdhoc, 		ParamDesc, 	0, "High Adhoc Mode"
HKR,Ndi\params\11nAdhoc, 		type, 		0, "enum"
HKR,Ndi\params\11nAdhoc, 		default, 	0, "0"
HKR,Ndi\params\11nAdhoc\enum, 	"0", 		0, "Disable"
HKR,Ndi\params\11nAdhoc\enum, 	"1", 		0, "Enable"
HKR,defaults,11nAdhoc, 0, "0"
HKR,,11nAdhoc, 0, "0"

;;----------------------------------------------------------------------------
;; Usb selective suspend parameters
;;----------------------------------------------------------------------------
[NdisSS.reg]
HKR,Ndi\params\*SelectiveSuspend,	    ParamDesc,  0, %SelectiveSuspend%
HKR,Ndi\params\*SelectiveSuspend,	    default,    0, "1"
HKR,Ndi\params\*SelectiveSuspend,	    type,       0, "enum"
HKR,Ndi\params\*SelectiveSuspend\enum,   "0",        0, "Disabled"
HKR,Ndi\params\*SelectiveSuspend\enum,   "1",        0, "Enabled"

HKR,Ndi\params\*SSIdleTimeout,	    ParamDesc,  0, %SSIdleTimeout%
HKR,Ndi\params\*SSIdleTimeout,	    type,       0, "int"
HKR,Ndi\params\*SSIdleTimeout,	    default,    0, "10"
HKR,Ndi\Params\*SSIdleTimeout,      Max,        0, "60"
HKR,Ndi\Params\*SSIdleTimeout,      Min,        0, "5"
HKR,Ndi\Params\*SSIdleTimeout,      Step,       0, "1"

HKR,,*SSIdleTimeout, 0, "10"


;*******************************************************************************
; bandwidth setting
;*******************************************************************************
[2G40MHzAnd5G40MHz.reg]
HKR,Ndi\params\BW40MHzFor2G,        ParamDesc,  0, "Bandwidth_2.4G"
HKR,Ndi\params\BW40MHzFor2G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor2G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor2G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor2G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,,"1"

HKR,Ndi\params\BW40MHzFor5G,        ParamDesc,  0, "Bandwidth_5G"
HKR,Ndi\params\BW40MHzFor5G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor5G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

[2G20MHzAnd5G40MHz.reg]
HKR,defaults,BW40MHzFor2G,0,"0"
HKR,,BW40MHzFor2G,0,"0"

HKR,Ndi\params\BW40MHzFor5G,        ParamDesc,  0, "Bandwidth_5G"
HKR,Ndi\params\BW40MHzFor5G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor5G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

[2G20MHzAnd5G20MHz.reg]
HKR,defaults,BW40MHzFor2G,0,"0"
HKR,,BW40MHzFor2G,0,"0"

HKR,defaults,BW40MHzFor5G,0,"0"
HKR,,BW40MHzFor5G,0,"0"

[BandWidthSetting.reg]
;; 40MHz Support in 11n
HKR,Ndi\params\BWSetting,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BWSetting,        type,       0, "enum"
HKR,Ndi\params\BWSetting,        default,    0, "1"
HKR,Ndi\params\BWSetting\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum,   "1",        0, "20_40MHz"
HKR,defaults,BWSetting,0,"1"
HKR,,BWSetting,0,"1"
HKR,,BWSetting,,"1"

[BelkinCustomId.reg]
HKR,,CustomerID,0,"21"
HKR,,CustomerID,,"21"

[BandSet.reg]
HKR,Ndi\params\WirelessBand,			ParamDesc,  0, "Disable Bands"
HKR,Ndi\params\WirelessBand,			type,       0, "enum"
HKR,Ndi\params\WirelessBand,			default,    0, "0"
HKR,Ndi\params\WirelessBand\enum,		"0",        0, "Disable 11A"
HKR,Ndi\params\WirelessBand\enum,		"1",        0, "Disable 11B/G"
HKR,Ndi\params\WirelessBand\enum,		"2",        0, "None"
HKR,defaults,WirelessBand,0,"2"
HKR,,WirelessBand,0,"2"

[BandOnly5G.reg]
HKR,defaults,WirelessBand,0,"1"
HKR,,WirelessBand,0,"1"


;*****************************************************************************
; For Wifi config
;*****************************************************************************
[WifiConfig.reg]
;; For WiFi test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\WiFiConfg,        ParamDesc,  0, "WiFi Config"
HKR,Ndi\params\WiFiConfg,        type,       0, "enum"
HKR,Ndi\params\WiFiConfg,        default,    0, "0"
HKR,Ndi\params\WiFiConfg\enum,   "0",        0, "Performance"
HKR,Ndi\params\WiFiConfg\enum,   "1",        0, "WiFi"
HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"
HKR,,WiFiConfg,,"0"

[Disable8021X_WifiConfig.reg]
;; For WiFi test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\WiFiConfg,        ParamDesc,  0, "WiFi Config"
HKR,Ndi\params\WiFiConfg,        type,       0, "enum"
HKR,Ndi\params\WiFiConfg,        default,    0, "0"
HKR,Ndi\params\WiFiConfg\enum,   "0",        0, "Performance"
HKR,Ndi\params\WiFiConfg\enum,   "1",        0, "WiFi"
HKR,Ndi\params\WiFiConfg\enum,   "2",        0, "Disable 802.1x"
HKR,defaults,WiFiConfg,0,"2"
HKR,,WiFiConfg,0,"2"
HKR,,WiFiConfg,,"2"


;;----------------------------------------------------------------------------
;; 8811AU/8821AU WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTL8811AU_COMMON.reg]
HKR,,EnableTxPowerLimit,0,"0"
HKR,,TxDutyEnable,0,"1"
HKR,,StbcCap,0,"17"
HKR,,RxSPStream,0,"1"
HKR,,RspPwr, 0, "1"

;; 8811AU support VHT24G mode.
HKR,Ndi\params\Vht24g, 		ParamDesc, 	0, "VHT 2.4G IOT"
HKR,Ndi\params\Vht24g, 		type, 		0, "enum"
HKR,Ndi\params\Vht24g, 		default, 	0, "255"
HKR,Ndi\params\Vht24g\enum, 	"0", 		0, "Disable"
HKR,Ndi\params\Vht24g\enum, 	"255", 		0, "Enable"
HKR,Ndi\params\Vht24g\enum, 	"254", 		0, "Not support Broadcom vendor"
HKR,defaults,Vht24g, 0, "255"
HKR,,Vht24g, 0, "255"

HKR,defaults,UsbTxAggDescNum,0,"10"
HKR,,UsbTxAggDescNum,0,"10"

HKR,,DecryptCustomFile,,"1"
HKR,,PwrByRateFile,0,"EncPWT.txt"
HKR,,PwrLimitFile,0,"TXPWR_LMT.txt"

HKR,,LdpcCap,0,"34"

HKR,,HWRTSEnable,,"1"

HKR,,BeamformCap,0,"34"

;;----------------------------------------------------------------------------
;; KFree parameters
;;----------------------------------------------------------------------------
[KFREE_COMMON.reg]
HKR,,RfKFreeEnable,0,"0"

;;----------------------------------------------------------------------------
;; Sniffer parameters
;;----------------------------------------------------------------------------
[AdvSniffer.reg]
HKR,,AdvanceSnifferMode,0,"8"

;;----------------------------------------------------------------------------
;; 8192EU WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTL8192EU_COMMON.reg]
HKR,defaults,UsbTxAggDescNum,0,"15"
HKR,,UsbTxAggDescNum,0,"15"
HKR,,DisableBTCoexist,0,"1"
HKR,,WoWLANMode, 0, "0"

HKR,,LdpcCap,0,"0"
HKR,,StbcCap,0,"48"
HKR,,BeamformCap,0,"48"

HKR,,bEarlymodeEnable,0,"0"

[DLINK_RTL8192EU_COMMON.reg]
HKR,defaults,UsbTxAggDescNum,0,"15"
HKR,,UsbTxAggDescNum,0,"15"
HKR,,DisableBTCoexist,0,"1"
HKR,,WoWLANMode, 0, "0"

HKR,,LdpcCap,0,"0"
HKR,,StbcCap,0,"48"
HKR,,BeamformCap,0,"48"

HKR,,bEarlymodeEnable,0,"0"
HKR,,SoftApAdaptivityNormal,0,"1"

[DisableSS.reg]
;; disable selective suspend.
HKR,defaults,NdisSS,0,"0"
HKR,,NdisSS,0,"0"

;;----------------------------------------------------------------------------
;; Actiontec WLAN NIC parameters
;;----------------------------------------------------------------------------
[Actiontec.reg]
HKR,defaults,VWifiSupport,0,"0"
HKR,,VWifiSupport,0,"0"

;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTWlanU.CopyFiles]
rtwlanu.sys,,,2

[DestinationDirs]
DefaultDestDir     	= 11
RTWlanU.CopyFiles	= 12

;;****************************************************************************
;; Source Files
;;****************************************************************************


[SourceDisksFiles]
rtwlanu.sys = 1

[SourceDisksNames]
1=%DISKNAME%,,,
;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
SSID_STR					= "SSID"
CHANNEL_STR					= "Channel"
NETWORK_TYPE_STR			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR						= "QoS"
WiFiConfg_STR	  			= "WiFiConfg"
WMM_APSD					= "WMM APSD"
CCX_RM_STR					= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
HW_PARA_STR					= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR						= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
DISABLE_STR					= "Disable"
ENABLE_STR					= "Enable"
AD_HOC_STR					= "Ad Hoc"
INFRASTRUCTURE_STR			= "Infrastructure"
AUTO_SELECT					= "Auto select"
WL_MODE_STR					= "Wireless Mode"
RX_REORDER_STR				= "Rx Reorder"
CAM_STR						= "CAM"
MAX_PSP_STR					= "MAX_PSP"
Fast_PSP_STR				= "Fast_PSP"
NO_AC_STR					= "No AC (Disable)"
ALL_AC_STR					= "ALL AC"
AUTO_STR 				= "Auto"
IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
IEEE_802_11AC_STR			= "IEEE 802.11ac"
SelectiveSuspend               		= "Selective suspend"
SSIdleTimeout                  		= "Selective suspend Timeout"

TX_PWR_CONTROL_STR		= "送信出力"
TX_PWR_PERCENTAGE_1_STR 	= "12.5%"
TX_PWR_PERCENTAGE_2_STR 	= "25%"
TX_PWR_PERCENTAGE_3_STR 	= "50%"
TX_PWR_PERCENTAGE_4_STR 	= "100%"
STREAM_MODE_STR			= "ストリーミングモード"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
PingPatternEnable           = "Wake on Pattern Match by Ping Pattern"
PacketCoalescing		= "D0 Packet Coalescing"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation strings
;-------------------------------------------------------------------------------
RX_AGG_MODE_STR				= "Rx Aggregation Mode"
RX_AGG_MODE_BLOCK_STR		= "Rx Agg USB Block Mode"
RX_AGG_MODE_PAGE_STR		= "Rx Agg DMA Page Mode"
RX_AGG_MODE_MIXED_STR		= "Rx Agg USB and Page Mixed Mode"
RX_AGG_USB_BLOCK_STR		= "Rx Agg USB Block Threshold"
RX_AGG_USB_TIMEOUT_STR		= "Rx Agg USB Timeout"
RX_AGG_DMA_PAGE_STR			= "Rx Agg DMA Page Threshold"
RX_AGG_DMA_TIMEOUT_STR		= "Rx Agg DMA Timeout"
TX_AGG_MODE_STR				= "Tx Aggregation Mode"
TX_AGG_DESC_PER_OUT_STR		= "Tx Agg Number of descriptor per bulk out"

;-------------------------------------------------------------------------------
;	Two STA Concurrent Mode
;-------------------------------------------------------------------------------
TWO_STA_CONCURRENT_MODE		= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"


;*******************************************************************************
; manufacture description
;*******************************************************************************
Realtek					= "Realtek Semiconductor Corp."
PCI             		= "PLANEX COMMUNICATIONS INC"
Sitecom         		= "Sitecom Europe B.V."
EDIMAX         			= "Edimax Technology Co., Ltd."
ELECOM         			= "ELECOM CO.,LTD."
Abocom					= "AboCom System, Inc."
Amigo					= "Amigo Technology Inc"
Hercules				= "Guillemot Corporation S.A"
DLink					= "D-Link Corporation"
Belkin					= "Belkin International, Inc."
Zyxel					= "ZyXEL"
ATKK					= "Allied Telesis K.K."
TRENDnet				= "TRENDnet"
Feixun					= "Shanghai Feixun Communication Co.,Ltd"
NetweeN					= "NetweeN"
XAVI					= "XAVI Technologies Corp."
Netgear					= "NETGEAR Inc."
Oar_Inc					= "Oar Inc."
ASUS					= "ASUSTeK Computer Inc."
HAWKING					= "Hawking Technologies Inc."
Compare					= "Compare Electronics CO.,LTD"
IO_DATA					= "I-O DATA DEVICE, INC"
TPLINK					= "TP-Link Technologies Co., Ltd."
Logitec					= "Logitec Japan"
NEC						= "NEC AccessTechnica, Ltd."
ACTIONTEC				= "Actiontec"
WD						= "Western Digital"
EnGenius				= "EnGenius Technologies."
Linksys					= "Linksys LLC"
BUFFALO					="BUFFALO INC."
Amped					= "Amped Wireless"
Qihoo					= "Qihoo 360 Technology Co.,Ltd"
Proxim					= "Proxim Wireless Corporation"
AirTies					= "AirTies Wireless Networks"
NETSCOUT				= "NETSCOUT Systems inc."
LiteOn					= "LITE-ON TECHNOLOGY CROP."
CCNC					= "CC&C Technologies. Inc."
;*******************************************************************************
;	Source disk name
;*******************************************************************************
;DISKNAME							= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
DISKNAME							= "Realtek Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
RtlWlanu.DeviceDesc 				= "Realtek Wireless LAN 802.11n USB 2.0 Network Adapter"
RtlWlanu.DeviceDesc.DispName		= "Realtek Wireless LAN 802.11n USB 2.0 Network Adapter"



;*******************************************************************************
; RTL8723bu Device description
;*******************************************************************************
RTL8723bu.DeviceDesc 				= "Realtek RTL8723B Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8723bu.DeviceDesc.DispName		= "Realtek RTL8723B Wireless LAN 802.11n USB 2.0 Network Adapter"
Edimax_N150.DeviceDesc				= "Edimax Wi-Fi N150 Bluetooth4.0 USB Adapter"
Edimax_N150.DeviceDesc.DispName		= "Edimax Wi-Fi N150 Bluetooth4.0 USB Adapter"
TRENDnet_108A.DeviceDesc	=	 "TRENDnet TBW-108UB N150 USB Network Adapter"
TRENDnet_108A.DeviceDesc.DispName	=	 "TRENDnet TBW-108UB N150 USB Network Adapter"
TRENDnet_808A.DeviceDesc	=	 "TRENDnet TEW-808UBM AC1200 Nano USB Adapter"
TRENDnet_808A.DeviceDesc.DispName	=	 "TRENDnet TEW-808UBM AC1200 Nano USB Adapter"

;*******************************************************************************
; RTL8703bu Device description
;*******************************************************************************
RTL8703bu.DeviceDesc 				= "Realtek RTL8703B Wireless LAN 802.11ac USB 2.0 Network Adapter"
RTL8703bu.DeviceDesc.DispName		= "Realtek RTL8703B Wireless LAN 802.11ac USB 2.0 Network Adapter"

;*******************************************************************************
; RTL8188fu Device description
;*******************************************************************************
RTL8188fu.DeviceDesc 				= "Realtek RTL8188FTV Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188fu.DeviceDesc.DispName		= "Realtek RTL8188FTV Wireless LAN 802.11n USB 2.0 Network Adapter"

;*******************************************************************************
; RTL8188EU Device description
;*******************************************************************************
RTL8188eu.DeviceDesc 				= "Realtek RTL8188EU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188eu.DeviceDesc.DispName		= "Realtek RTL8188EU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188ee_vau.DeviceDesc 			= "Realtek RTL8188EE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ee_vau.DeviceDesc.DispName	= "Realtek RTL8188EE-VAU Wireless LAN 802.11n USB minicard"
RTL8188eu_0179.DeviceDesc 			= "Realtek RTL8188ETV Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188eu_0179.DeviceDesc.DispName	= "Realtek RTL8188ETV Wireless LAN 802.11n USB 2.0 Network Adapter"
Abocom_8179.DeviceDesc 				= "802.11bgn Mini Wireless LAN USB2.0 Adapter"
Abocom_8179.DeviceDesc.DispName		= "802.11bgn Mini Wireless LAN USB2.0 Adapter"
DLINK_330F.DeviceDesc 				= "D-Link DWA-125 Wireless N 150 USB Adapter(rev.D)"
DLINK_330F.DeviceDesc.DispName		= "D-Link DWA-125 Wireless N 150 USB Adapter(rev.D)"
DLINK_3310.DeviceDesc 				= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.D)"
DLINK_3310.DeviceDesc.DispName		= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.D)"
DLINK_3311.DeviceDesc 				= "D-Link GO-USB-N150 Wireless N 150 Easy USB Adapter(rev.B)"
DLINK_3311.DeviceDesc.DispName		= "D-Link GO-USB-N150 Wireless N 150 Easy USB Adapter(rev.B)"
DLINK_331B.DeviceDesc 				= "D-Link DWA-121 Wireless N 150 USB Adapter(rev.B)"
DLINK_331B.DeviceDesc.DispName		= "D-Link DWA-121 Wireless N 150 USB Adapter(rev.B)"
ELECOM_4008.DeviceDesc				= "ELECOM WDC-150SU2M Wireless Adapter"
ELECOM_4008.DeviceDesc.DispName		= "ELECOM WDC-150SU2M Wireless Adapter"

;*******************************************************************************
; RTL8812AU Device description
;*******************************************************************************
RTL8812au.DeviceDesc 					= "Realtek 8812AU Wireless LAN 802.11ac USB NIC"
RTL8812au.DeviceDesc.DispName			= "Realtek 8812AU Wireless LAN 802.11ac USB NIC"
RTL8812au_881A.DeviceDesc 				= "RTL8812AU-VS(802.11ac 2x2 USB2.0)"
RTL8812au_881A.DeviceDesc.DispName		= "RTL8812AU-VS(802.11ac 2x2 USB2.0)"
RTL8812au_881B.DeviceDesc 				= "RTL8812AU-VL(802.11ac 1x1 USB2.0)"
RTL8812au_881B.DeviceDesc.DispName		= "RTL8812AU-VL(802.11ac 1x1 USB2.0)"
RTL8812au_881C.DeviceDesc 				= "RTL8812AU-VN(802.11n 2x2 USB2.0)"
RTL8812au_881C.DeviceDesc.DispName		= "RTL8812AU-VN(802.11n 2x2 USB2.0)"

Belkin-AC950.DeviceDesc					= "Belkin USB Wireless Adapter"
Belkin-AC950.DeviceDesc.DispName		= "Belkin USB Wireless Adapter"

Netgear-A6200v2.DeviceDesc              = "NETGEAR A6200V2 11AC Wireless USB 3.0 Adapter"
Netgear-A6200v2.DeviceDesc.DispName     = "NETGEAR A6200V2 11AC Wireless USB 3.0 Adapter"

DLink-DWA183.DeviceDesc                 = "D-Link DWA-183 Wireless AC Dual Band USB Adapter"
DLink-DWA183.DeviceDesc.DispName        = "D-Link DWA-183 Wireless AC Dual Band USB Adapter"
DLink-DWA182.DeviceDesc                 = "D-Link DWA-182 Wireless AC Dual Band USB Adapter(rev.B)"
DLink-DWA182.DeviceDesc.DispName        = "D-Link DWA-182 Wireless AC Dual Band USB Adapter(rev.B)"
DLink_3315.DeviceDesc                	= "Wireless AC1200 Dual Band USB Adapter"
DLink_3315.DeviceDesc.DispName        	= "Wireless AC1200 Dual Band USB Adapter"
DLink_3316.DeviceDesc                 	= "Wireless AC1200 Dual Band USB Adapter"
DLink_3316.DeviceDesc.DispName        	= "Wireless AC1200 Dual Band USB Adapter"

Edimax_A822.DeviceDesc 				= "Edimax AC1200 Wireless LAN USB Adapter"
Edimax_A822.DeviceDesc.DispName		= "Edimax AC1200 Wireless LAN USB Adapter"

Sitecom_0074.DeviceDesc 				= "Sitecom WiFi USB adapter AC1200"
Sitecom_0074.DeviceDesc.DispName		= "Sitecom WiFi USB adapter AC1200"

IO_DATA_0952.DeviceDesc					= "I-O DATA WN-AC867U Wireless LAN Adapter"
IO_DATA_0952.DeviceDesc.DispName		= "I-O DATA WN-AC867U Wireless LAN Adapter"
                                    	
Logitec_016E.DeviceDesc					= "Logitec AC866 Wireless USB Adapter"
Logitec_016E.DeviceDesc.DispName		= "Logitec AC866 Wireless USB Adapter"
                                    	
ASUS_17D2.DeviceDesc 					= "ASUS USB-AC56 802.11ac Wireless USB Adapter"
ASUS_17D2.DeviceDesc.DispName			= "ASUS USB-AC56 802.11ac Wireless USB Adapter"
                                    	
Hawking_0022.DeviceDesc 				= "Hawking USB Wireless-AC Network Adapter"
Hawking_0022.DeviceDesc.DispName		= "Hawking USB Wireless-AC Network Adapter"

NEC_0408.DeviceDesc						= "NEC AtermWL900U(PA-WL900U) Wireless Network Adapter"
NEC_0408.DeviceDesc.DispName			= "NEC AtermWL900U(PA-WL900U) Wireless Network Adapter"

Zyxel_3426.DeviceDesc					= "ZyXEL Wireless AC USB Adapter"
Zyxel_3426.DeviceDesc.DispName			= "ZyXEL Wireless AC USB Adapter"

WD_0632.DeviceDesc						= "WD My Net AC USB Adapter"
WD_0632.DeviceDesc.DispName				= "WD My Net AC USB Adapter"

EnGenius_0100.DeviceDesc				= "EnGenius 802.11ac Dual Band Wireless USB Adapter"
EnGenius_0100.DeviceDesc.DispName		= "EnGenius 802.11ac Dual Band Wireless USB Adapter"

Linksys_003F.DeviceDesc					= "Linksys WUSB6300"
Linksys_003F.DeviceDesc.DispName		= "Linksys WUSB6300"

Amped_9097.DeviceDesc					= "Amped Wireless ACA1 Wi-Fi Adapter"
Amped_9097.DeviceDesc.DispName			= "Amped Wireless ACA1 Wi-Fi Adapter"

PCI_AB30.DeviceDesc 				= "GW-900D"
PCI_AB30.DeviceDesc.DispName		= "GW-900D"

Abocom_8812.DeviceDesc 				= "802.11ac Wireless LAN Card"
Abocom_8812.DeviceDesc.DispName		= "802.11ac Wireless LAN Card"

TRENDnet_805B.DeviceDesc 			= "AC1200  Dual Band Wireless USB Adapter"
TRENDnet_805B.DeviceDesc.DispName		= "AC1200  Dual Band Wireless USB Adapter"

Buffalo_025D.DeviceDesc				= "BUFFALO WI-U3-866D Wireless LAN Adapter"
Buffalo_025D.DeviceDesc.DispName		= "BUFFALO WI-U3-866D Wireless LAN Adapter"

Proxim_0115.DeviceDesc				= "ORiNOCO 802.11a/b/g/n/ac USB Adapter"
Proxim_0115.DeviceDesc.DispName		= "ORiNOCO 802.11a/b/g/n/ac USB Adapter"

;*******************************************************************************
; TP-Link General Device description
;*******************************************************************************
TPLINK_0101.DeviceDesc					= "TP-Link Wireless USB Adapter"
TPLINK_0101.DeviceDesc.DispName			= "TP-Link Wireless USB Adapter"

TPLINK_0117.DeviceDesc					= "TP-Link High Power Wireless USB Adapter"
TPLINK_0117.DeviceDesc.DispName			= "TP-Link High Power Wireless USB Adapter"

;*******************************************************************************
; RTL8811AU Device description
;*******************************************************************************
RTL8811au.DeviceDesc					= "Realtek RTL8811AU Wireless LAN 802.11ac USB 2.0 Network Adapter"
RTL8811au.DeviceDesc.DispName			= "Realtek RTL8811AU Wireless LAN 802.11ac USB 2.0 Network Adapter"
RTL8811au_Combo.DeviceDesc					= "Realtek RTL8821AU Wireless LAN 802.11ac USB 2.0 Network Adapter"
RTL8811au_Combo.DeviceDesc.DispName			= "Realtek RTL8821AU Wireless LAN 802.11ac USB 2.0 Network Adapter"

Buffalo-WI-U2-433DM.DeviceDesc 						= "BUFFALO WI-U2-433DM Wireless LAN Adapter"
Buffalo-WI-U2-433DM.DeviceDesc.DispName 		= "BUFFALO WI-U2-433DM Wireless LAN Adapter"

Buffalo_029B.DeviceDesc 				= "BUFFALO WI-U2-433DHP Wireless Lan Adapter"
Buffalo_029B.DeviceDesc.DispName 		= "BUFFALO WI-U2-433DHP Wireless Lan Adapter"

Buffalo_029D.DeviceDesc 				= "BUFFALO WLP-U2-433DHP Wireless Lan Adapter"
Buffalo_029D.DeviceDesc.DispName 		= "BUFFALO WLP-U2-433DHP Wireless Lan Adapter"

Edimax_AC600.DeviceDesc					= "Edimax AC600 Wireless LAN USB Adapter"
Edimax_AC600.DeviceDesc.DispName		= "Edimax AC600 Wireless LAN USB Adapter"

ELECOM_WDC433DU2.DeviceDesc				= "ELECOM WDC-433DU2H 11ac Wireless Adapter"
ELECOM_WDC433DU2.DeviceDesc.DispName	= "ELECOM WDC-433DU2H 11ac Wireless Adapter"

ELECOM_WDC433SU2M2.DeviceDesc			= "ELECOM WDC-433SU2M2  Wireless Adapter"
ELECOM_WDC433SU2M2.DeviceDesc.DispName	= "ELECOM WDC-433SU2M2  Wireless Adapter"
ELECOM_WDB433SU2M2.DeviceDesc			= "ELECOM WDB-433SU2M2  Wireless Adapter"
ELECOM_WDB433SU2M2.DeviceDesc.DispName	= "ELECOM WDB-433SU2M2  Wireless Adapter"

Hawking_0023.DeviceDesc					= "Hawking USB WLS 11AC Adapter"
Hawking_0023.DeviceDesc.DispName		= "Hawking USB WLS 11AC Adapter"

IO_DATA_AC433UA.DeviceDesc					= "I-O DATA WN-AC433UA Wireless LAN Adapter"
IO_DATA_AC433UA.DeviceDesc.DispName		= "I-O DATA WN-AC433UA Wireless LAN Adapter"

DLink-DWA171.DeviceDesc	=	 "D-Link DWA-171 Wireless AC Dual Band Adapter"
DLink-DWA171.DeviceDesc.DispName	=	 "D-Link DWA-171 Wireless AC Dual Band Adapter"
DLink_3318.DeviceDesc	=	 "Wireless AC600 Dual Band High-Gain USB Adapter"
DLink_3318.DeviceDesc.DispName	=	 "Wireless AC600 Dual Band High-Gain USB Adapter"

TRENDnet_804B.DeviceDesc	=	 "AC600 Dual Band Wireless USB Adapter"
TRENDnet_804B.DeviceDesc.DispName	=	 "AC600 Dual Band Wireless USB Adapter"

PCI_AB32.DeviceDesc					=	"GW-450S"
PCI_AB32.DeviceDesc.DispName		=	"GW-450S"

Sitecom_007A.DeviceDesc 				= "WiFi High Gain USB Adapter AC600"
Sitecom_007A.DeviceDesc.DispName		= "WiFi High Gain USB Adapter AC600"

IO_DATA_0959.DeviceDesc					=	"I-O DATA WN-AC433UM Wireless LAN Adapter"
IO_DATA_0959.DeviceDesc.DispName		=	"I-O DATA WN-AC433UM Wireless LAN Adapter"
IO_DATA_095A.DeviceDesc					=	"I-O DATA WHG-AC433UM Wireless LAN Adapter"
IO_DATA_095A.DeviceDesc.DispName		=	"I-O DATA WHG-AC433UM Wireless LAN Adapter"

IO_DATA_2003.DeviceDesc					=	"Realtek Wireless LAN USB 2.0 5G Only Network Adapter"
IO_DATA_2003.DeviceDesc.DispName		=	"Realtek Wireless LAN USB 2.0 5G Only Network Adapter"

AirTies_2520.DeviceDesc					=	"AirTies Air2520 Wireless USB Adapter"
AirTies_2520.DeviceDesc.DispName		=	"AirTies Air2520 Wireless USB Adapter"
AirTies_2525.DeviceDesc					=	"AirTies Air2525 Wireless USB Adapter"
AirTies_2525.DeviceDesc.DispName		=	"AirTies Air2525 Wireless USB Adapter"

Abocom_0811.DeviceDesc 				= "802.11ac Wireless LAN Card"
Abocom_0811.DeviceDesc.DispName		= "802.11ac Wireless LAN Card"


;*******************************************************************************
; RTL8192E Device description
;*******************************************************************************
RTL8192eu.DeviceDesc					= "Realtek RTL8192EU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192eu.DeviceDesc.DispName			= "Realtek RTL8192EU Wireless LAN 802.11n USB 2.0 Network Adapter"
DLink_2001.DeviceDesc					= "D-Link DWA-131 Wireless N Nano USB Adapter"
DLink_2001.DeviceDesc.DispName			= "D-Link DWA-131 Wireless N Nano USB Adapter"
Abocom_AB33.DeviceDesc				= "GW-300S KATANA"
Abocom_AB33.DeviceDesc.DispName		= "GW-300S KATANA"

;*******************************************************************************
; RTL8814AU Device description
;*******************************************************************************
RTL8814au.DeviceDesc 					= "Realtek 8814AU Wireless LAN 802.11ac USB NIC"
RTL8814au.DeviceDesc.DispName			= "Realtek 8814AU Wireless LAN 802.11ac USB NIC"
DLink_331A.DeviceDesc 					= "D-Link DWA-192 AC1900 Wi-Fi USB 3.0 Adapter"
DLink_331A.DeviceDesc.DispName			= "D-Link DWA-192 AC1900 Wi-Fi USB 3.0 Adapter"
ASUS_1817.DeviceDesc 					= "ASUS USB-AC68 USB Wireless adapter"
ASUS_1817.DeviceDesc.DispName			= "ASUS USB-AC68 USB Wireless adapter"
ASUS_1852.DeviceDesc 					= "ASUS USB-AC68 USB Wireless adapter"
ASUS_1852.DeviceDesc.DispName			= "ASUS USB-AC68 USB Wireless adapter"
ASUS_1853.DeviceDesc 					= "ASUS USB-AC68 USB Wireless adapter"
ASUS_1853.DeviceDesc.DispName			= "ASUS USB-AC68 USB Wireless adapter"
ELECOM_WDC1300DU3.DeviceDesc			= "ELECOM WDC-1300DU3 Wireless Adapter"
ELECOM_WDC1300DU3.DeviceDesc.DispName	= "ELECOM WDC-1300DU3 Wireless Adapter"
ELECOM_WDC1300SU3.DeviceDesc			= "ELECOM WDC-1300SU3 Wireless Adapter"
ELECOM_WDC1300SU3.DeviceDesc.DispName	= "ELECOM WDC-1300SU3 Wireless Adapter"
Edimax_AC1750.DeviceDesc							= "Edimax AC1750 Wi-Fi USB Adapter"
Edimax_AC1750.DeviceDesc.DispName		= "Edimax AC1750 Wi-Fi USB Adapter"
Sitecom_007B.DeviceDesc							= "WiFi USB adapter AC1750"
Sitecom_007B.DeviceDesc.DispName			= "WiFi USB adapter AC1750"
TRENDnet_809A.DeviceDesc	=	 "TRENDnet TEW-809UB AC1900 Wireless USB Adapter"
TRENDnet_809A.DeviceDesc.DispName	=	 "TRENDnet TEW-809UB AC1900 Wireless USB Adapter"
Netscout_0002.DeviceDesc	=	"NETSCOUT 802.11ac USB Network Adapter"
Netscout_0002.DeviceDesc.DispName	=	"NETSCOUT 802.11ac USB Network Adapter"
Hawking_0026.DeviceDesc					= "Hawking HW17ACU USB AC Adapter"
Hawking_0026.DeviceDesc.DispName		= "Hawking HW17ACU USB AC Adapter"

;*******************************************************************************
; RTL8822BU Device description
;*******************************************************************************
RTL8822bu.DeviceDesc 					= "Realtek 8822BU Wireless LAN 802.11ac USB NIC"
RTL8822bu.DeviceDesc.DispName			= "Realtek 8822BU Wireless LAN 802.11ac USB NIC"
RTL8812bu.DeviceDesc					= "Realtek 8812BU Wireless LAN 802.11ac USB NIC"
RTL8812bu.DeviceDesc.DispName			= "Realtek 8812BU Wireless LAN 802.11ac USB NIC"
LITEON_8602.DeviceDesc					= "WN8602L Wireless LAN 802.11ac USB NIC"
LITEON_8602.DeviceDesc.DispName			= "WN8602L Wireless LAN 802.11ac USB NIC"
CC_2102.DeviceDesc						= "CC&C 433Mbps Wireless USB2.0 Adapter"
CC_2102.DeviceDesc.DispName				= "CC&C 433Mbps Wireless USB2.0 Adapter"
ASUS_1841.DeviceDesc					= "ASUS USB Wireless Adapter"
ASUS_1841.DeviceDesc.DispName			= "ASUS USB Wireless Adapter"
ASUS_184C.DeviceDesc					= "ASUS USB-AC53 Nano USB Wireless adapter"
ASUS_184C.DeviceDesc.DispName			= "ASUS USB-AC53 Nano USB Wireless adapter"
ASUS_1870.DeviceDesc					= "ASUS USB Wireless Adapter"
ASUS_1870.DeviceDesc.DispName			= "ASUS USB Wireless Adapter"
ASUS_1874.DeviceDesc					= "ASUS USB Wireless Adapter"
ASUS_1874.DeviceDesc.DispName			= "ASUS USB Wireless Adapter"
DLINK_331C.DeviceDesc 				= "D-Link DWA-182 Wireless AC 1200 USB Adapter(rev.D)"
DLINK_331C.DeviceDesc.DispName		= "D-Link DWA-182 Wireless AC 1200 USB Adapter(rev.D)"
Linksys_0043.DeviceDesc					= "2X2 selectable dual-band 802.11ac USB network adapter"
Linksys_0043.DeviceDesc.DispName		= "2X2 selectable dual-band 802.11ac USB network adapter"
Edimax_C822.DeviceDesc				= "Edimax AC1200 MU-MIMO WiFi USB 3.0 Adapter"
Edimax_C822.DeviceDesc.DispName		= "Edimax AC1200 MU-MIMO WiFi USB 3.0 Adapter"
Edimax_B822.DeviceDesc				= "Edimax AC1200 MU-MIMO WiFi Nano USB 2.0 Adapter"
Edimax_B822.DeviceDesc.DispName		= "Edimax AC1200 MU-MIMO WiFi Nano USB 2.0 Adapter"
Edimax_D822.DeviceDesc				= "Dacota Platinum AC1200 USB 2.0 Wireless Adapter"
Edimax_D822.DeviceDesc.DispName		= "Dacota Platinum AC1200 USB 2.0 Wireless Adapter"
Edimax_E822.DeviceDesc				= "Dacota Platinum AC1200 USB 3.0 Wireless Adapter"
Edimax_E822.DeviceDesc.DispName		= "Dacota Platinum AC1200 USB 3.0 Wireless Adapter"
Hawking_0025.DeviceDesc					= "Hawking HW12ACU USB AC Adapter"
Hawking_0025.DeviceDesc.DispName		= "Hawking HW12ACU USB AC Adapter"
TPLINK_012D.DeviceDesc					= "TP-Link Wireless Mini MU-MIMO USB Adapter"
TPLINK_012D.DeviceDesc.DispName			= "TP-Link Wireless Mini MU-MIMO USB Adapter"
TPLINK_012E.DeviceDesc					= "TP-Link Wireless Mini MU-MIMO USB Adapter"
TPLINK_012E.DeviceDesc.DispName			= "TP-Link Wireless Mini MU-MIMO USB Adapter"
TPLINK_0115.DeviceDesc					= "TP-Link Wireless MU-MIMO USB Adapter"
TPLINK_0115.DeviceDesc.DispName			= "TP-Link Wireless MU-MIMO USB Adapter"


;*******************************************************************************
; RTL8821CU Device description
;*******************************************************************************
RTL8821cu.DeviceDesc 					= "Realtek 8821CU Wireless LAN 802.11ac USB NIC"
RTL8821cu.DeviceDesc.DispName			= "Realtek 8821CU Wireless LAN 802.11ac USB NIC"

;*******************************************************************************
; RTL8811CU Device description
;*******************************************************************************
RTL8811cu.DeviceDesc 					= "Realtek 8811CU Wireless LAN 802.11ac USB NIC"
RTL8811cu.DeviceDesc.DispName			= "Realtek 8811CU Wireless LAN 802.11ac USB NIC"
ZION_2006.DeviceDesc					= "TOTOLINK Wireless Adapter"
ZION_2006.DeviceDesc.DispName			= "TOTOLINK Wireless Adapter"
DLINK_331D.DeviceDesc 					= "D-Link DWA-171 AC600 MU-MIMO Wi-Fi USB Adapter"
DLINK_331D.DeviceDesc.DispName			= "D-Link DWA-171 AC600 MU-MIMO Wi-Fi USB Adapter"
TPLINK_012C.DeviceDesc					= "TP-Link Wireless Nano MU-MIMO USB Adapter"
TPLINK_012C.DeviceDesc.DispName			= "TP-Link Wireless Nano MU-MIMO USB Adapter"

;*******************************************************************************
; RTL8723DU Device description
;*******************************************************************************
RTL8723du.DeviceDesc 					= "Realtek 8723DU Wireless LAN 802.11n USB NIC"
RTL8723du.DeviceDesc.DispName			= "Realtek 8723DU Wireless LAN 802.11n USB NIC"

;*******************************************************************************
; RTL8710BU Device description
;*******************************************************************************
RTL8710bu.DeviceDesc 					= "Realtek 8188GU Wireless LAN 802.11n USB NIC"
RTL8710bu.DeviceDesc.DispName			= "Realtek 8188GU Wireless LAN 802.11n USB NIC"
ZION_2005.DeviceDesc					= "TOTOLINK Wireless Adapter"
ZION_2005.DeviceDesc.DispName			= "TOTOLINK Wireless Adapter"
